Project Name:	NAR
	Project Code:	NAR	Site ID:	B747	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	11/05/71	Elevation:	 220 metres
	Map Ref.:	Sheet No. : 9046   1:100000	Rainfall:	716
	Northing/Long.:	150.902777777778	Runoff:	No Data
	Easting/Lat.:	-25.7041666666667	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRt	Substrate Material:	Auger boring, 0.5 m deep,Adamellite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr4.23
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Heteropogon contortus
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Granular; 
	Dry; Very weak consistence; 20-50%, medium gravelly, 6-20mm, angular, Gravel, coarse 
	fragments; Field pH 8 (pH meter); Many, very fine (0-1mm) roots; Clear change to - 
	A2	0.1 - 0.25 m	Reddish brown (5YR4/3-Moist); Reddish brown (5YR5/3-Dry); ; Clayey coarse sand; Massive 
	grade of structure; Dry; Very weak consistence; 50-90%, coarse gravelly, 20-60mm, angular, 
	Gravel, coarse fragments; Field pH 8.3 (pH meter); Common, very fine (0-1mm) roots; Abrupt 
	change to - 
	B2	0.25 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Light clay; Massive grade of structure; Moderately moist; Firm 
	consistence; 20-50%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Field pH 
	8.5 (pH meter); Few, very fine (0-1mm) roots; Clear change to - 
	BC	0.3 - 0.4 m	Red (2.5YR5/5-Moist); , 5YR55, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Sandy 
	clay loam; Massive grade of structure; Dry; Firm consistence; 20-50%, medium gravelly, 6-
	20mm, angular, Gravel, coarse fragments; Field pH 8.5 (pH meter); Few, very fine (0-1mm) roots; 
	Gradual change to - 
	C	0.4 - 0.5 m	Yellowish red (5YR5/5-Moist); , 7.5YR86, 20-50% , 0-5mm, Prominent; , 10YR41, 20-50% , 0-
	5mm, Prominent; Sandy loam; Massive grade of structure; Dry; Very firm consistence; 20-50%, 
	coarse gravelly, 20-60mm, angular, Gravel, coarse fragments; Field pH 8 (pH meter); Few, very 
	fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	0-10CM POROUS GRANULAR STRUCTURE. BELOW 30CM MODERATE INCREASING TO STRONG MINERAL SPECKLING 
	PALE YELLOW WHITE ETC.     GRAVELS DOMINANTLY FELDSPAR.
	Site Notes
	NARAYEN

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B747	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.7H	 0.06B	 10.4K	 1.4	 0.61	 0.25	 5.7D
	0.1 - 0.25
	0.25 - 0.3
	0.3 - 0.4	8.1H	 0.02B	 5.2K	 2	 0.1	 0.2	 1.9D
	0.4 - 0.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.56A	 1160F	 0.225B	 2.7B	 52	 43C	 29	 8	 13
	0.1 - 0.25
	0.25 - 0.3
	0.3 - 0.4	 390F	 2.5B	 33	 50C	 25	 10	 16
	0.4 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.3
	0.3 - 0.4
	0.4 - 0.5

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B747	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded