Project Name:	NAR
	Project Code:	NAR	Site ID:	B795	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:	Catchment 4.
	Date Desc.:	20/09/72	Elevation:	 240 metres
	Map Ref.:	Sheet No. : 9046   1:100000	Rainfall:	716
	Northing/Long.:	150.910833333333	Runoff:	Moderately rapid
	Easting/Lat.:	-25.6922222222222	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRt	Substrate Material:	Undisturbed soil core, 0.7 m 
	deep,Adamellite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.21
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Heteropogon contortus, Aristida species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Coarse sandy loam; Massive grade of structure; Dry; Very weak 
	consistence; 20-50%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; Common, 
	very fine (0-1mm) roots; Gradual change to - 
	A1	0.1 - 0.15 m	Dark reddish brown (5YR3/2-Moist); ; Loamy coarse sand; Massive grade of structure; Dry; Very 
	weak consistence; 20-50%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; 
	Common, very fine (0-1mm) roots; Clear change to - 
	A2	0.15 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Loamy coarse sand; Massive grade of structure; Dry; Very 
	weak consistence; 50-90%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; Few, 
	very fine (0-1mm) roots; Clear change to - 
	A2	0.2 - 0.24 m	Dark reddish brown (5YR3/4-Moist); ; Clayey coarse sand; Massive grade of structure; Dry; Very 
	weak consistence; 50-90%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; Few, 
	very fine (0-1mm) roots; Abrupt, Wavy change to - 
	B2	0.24 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Weak grade of structure, 50-100 mm, Prismatic; 
	Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very firm consistence; 20-50%, fine
	 gravelly, 2-6mm, angular, Quartz, coarse fragments; Common, very fine (0-1mm) roots; 
	B2	0.3 - 0.52 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Weak grade of structure, 50-100 mm, Prismatic; 
	Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very firm consistence; 10-20%, fine
	 gravelly, 2-6mm, angular, Quartz, coarse fragments; Common, very fine (0-1mm) roots; Gradual 
	change to - 
	B2	0.52 - 0.6 m	Dark red (2.5YR3/6-Moist); , 10YR84, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; 
	Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Dry; Very firm consistence; 20-50%, fine gravelly, 2-6mm, 
	angular, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 
	B3	0.6 - 0.65 m	Dark red (2.5YR3/6-Moist); , 10YR84, 20-50% , 0-5mm, Prominent; , 20-50% , 0-5mm, Prominent;
	 Light medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Dry; Very firm consistence; 20-50%, fine gravelly, 2-6mm, 
	angular, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B795	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B3	0.65 - 0.7 m	Reddish brown (5YR4/4-Moist); , 2.5YR36, 10-20% , 0-5mm, Distinct; , 10YR84, 10-20% , 0-
	5mm, Distinct; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; Dry; Very firm 
	consistence; 20-50%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few, very fine (0-
	1mm) roots; Abrupt change to - 
	C	0.7 - 0.9 m	Dark red (2.5YR3/6-Moist); , 10YR54, 10-20% , 5-15mm, Distinct; , 10YR82, 10-20% , 5-15mm, 
	Distinct; Coarse sandy clay loam; Massive grade of structure; Dry; Very firm consistence; 20-
	50%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few, very fine (0-1mm) roots; 
	C	0.9 - 0.95 m	Dark red (2.5YR3/6-Moist); , 10YR54, 10-20% , 5-15mm, Distinct; , 10YR82, 10-20% , 5-15mm, 
	Distinct; Clayey coarse sand; Massive grade of structure; Dry; Very firm consistence; 20-50%, 
	fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	MUCH 10-25MM FELDSPAR GRAVEL IN A HORIZONS, BELOW 60CM PROMINENT MINERAL SPECKLING. 70-90CM ROCK 
	WEATHERED IN SITU.     LAYERS RENUMBERED 6-10-92
	Site Notes
	NARAYEN

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B795	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.8H	 0.035A	 4.4K	 1.2	 0.31	 0.04	 2.1D
	0.1 - 0.15	6.8H	<0.03A
	0.15 - 0.2	6.8H	<0.03A
	0.2 - 0.24	6.7H	<0.03A
	0.24 - 0.3	6.1H	<0.03A
	0.3 - 0.52	6.1H	<0.03A	 5.6K	 3	 0.34	 0.16	 7.5D
	0.52 - 0.6	6.4H	<0.03A
	0.6 - 0.65	6.5H	<0.03A
	0.65 - 0.7	6.8H	<0.03A
	0.7 - 0.9	7.3H	<0.03A
	0.9 - 0.95	7.3H	<0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.94A	 57B	 340F	 0.061B	 3.28B	1.00	 31	 56C	 27	 10	 8
	0.1 - 0.15	 0.58A	 32B	 0.04B	1.40	 45	 56C	 29	 9	 7
	0.15 - 0.2	 0.38A	 30B	 280F	 0.03B	 3.48B	1.60	 79	 62C	 24	 9	 7
	0.2 - 0.24	 0.25A	 10B	 0.025B	1.30	 74	 67C	 18	 5	 9
	0.24 - 0.3	 0.48A	 0.056B	1.50	 32	 47C	 13	 6	 35
	0.3 - 0.52	 0.45A	 3B	 340F	 0.045B	 2.48B	1.30	 21	 34C	 13	 6	 49
	0.52 - 0.6	1.10	 28	 33C	 17	 6	 44
	0.6 - 0.65	1.60	 23	 40C	 17	 7	 36
	0.65 - 0.7	2.00	 33	 46C	 21	 9	 24
	0.7 - 0.9	 3B	1.90	 27	 57C	 18	 9	 18
	0.9 - 0.95	1.90	 50	 75C	 15	 6	 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.24
	0.24 - 0.3
	0.3 - 0.52
	0.52 - 0.6
	0.6 - 0.65
	0.65 - 0.7
	0.7 - 0.9
	0.9 - 0.95

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B795	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded