Project Name:	NAR
	Project Code:	NAR	Site ID:	B798	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:	Catchment 3.
	Date Desc.:	20/09/72	Elevation:	 226 metres
	Map Ref.:	Sheet No. : 9046   1:100000	Rainfall:	716
	Northing/Long.:	150.904166666667	Runoff:	No Data
	Easting/Lat.:	-25.7	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRt	Substrate Material:	Undisturbed soil core, 1 m 
	deep,Unconsolidated material 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	30 metres
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Brown Chromosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Heteropogon contortus, Aristida species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Very dark brown (10YR2/2-Moist); ; Coarse sandy loam; Massive grade of structure; Dry; Firm 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Many, very fine 
	(0-1mm) roots; Clear change to - 
	A12	0.05 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Loamy coarse sand; Massive grade of structure; Dry; Firm 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Many, very fine 
	(0-1mm) roots; Clear change to - 
	A2	0.1 - 0.2 m	Greyish brown (10YR5/2-Moist); ; Coarse sand; Massive grade of structure; Dry; Firm 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Many, very fine 
	(0-1mm) roots; Gradual change to - 
	A2	0.2 - 0.3 m	Light brownish grey (10YR6/2-Moist); ; Coarse sand; Massive grade of structure; Dry; Weak 
	consistence; 20-50%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Many, very 
	fine (0-1mm) roots; Gradual change to - 
	A2	0.3 - 0.34 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/2-Dry); ; Coarse sand; Massive grade of 
	structure; Dry; Weak consistence; 20-50%, medium gravelly, 6-20mm, angular, Gravel, coarse 
	fragments; Common, very fine (0-1mm) roots; Sharp change to - 
	B21	0.34 - 0.47 m	Yellowish brown (10YR5/4-Moist); , 7.5YR56, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, 
	Distinct; Medium clay; Strong grade of structure, 100-200 mm, Columnar; Moderate grade of 
	structure, 10-20 mm, Polyhedral; Dry; Strong consistence; 20-50%, fine gravelly, 2-6mm, 
	angular, Gravel, coarse fragments; Common, very fine (0-1mm) roots; 
	B21	0.47 - 0.6 m	Greyish brown (2.5Y5/3-Moist); , 7.5YR58, 20-50% , 15-30mm, Distinct; , 20-50% , 15-30mm, 
	Distinct; Medium clay; Strong grade of structure, 100-200 mm, Columnar; Moderate grade of 
	structure, 10-20 mm, Polyhedral; Dry; Strong consistence; 20-50%, fine gravelly, 2-6mm, 
	angular, Gravel, coarse fragments; Common, very fine (0-1mm) roots; Diffuse change to - 
	B22	0.6 - 0.76 m	Greyish brown (10YR5/2-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, 
	Prominent; Light medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Dry; 
	Strong consistence; 20-50%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Very
	 few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; Few, very fine (0-1mm) roots; 

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B798	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	0.76 - 0.9 m	Greyish brown (10YR5/2-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; Dry; Strong 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Medium (2 -6 mm), Nodules; Diffuse change to - 
	B3	0.9 - 1.02 m	Brown (10YR5/3-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, 
	Prominent; Light clay; Weak grade of structure, 50-100 mm, Angular blocky; Dry; Strong 
	consistence; 20-50%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Few (2 - 10 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; 
	C	1.02 - 1.2 m	Strong brown (7.5YR5/6-Moist); , 2.5Y62, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Coarse sandy clay loam; Massive grade of structure; Dry; Very firm consistence; 20-
	50%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Few (2 - 10 %), 
	Manganiferous, Coarse (6 - 20 mm), Nodules; 
	Morphological Notes
	Observation Notes
	PARENT MATERIAL COLLUVIUM FROM ADAMELLITE. GRAVELS BOTH QUARTZ AND FELDSPAR. SOME SAND FILLED 
	FISSUES BETWEEN COLUMNS   EXTEND TO 90CM. B HORIZON PEDS HAVE 10YR4/2 STAINED FACES. LAYERS 
	RENUMBERED 6-10-92
	Site Notes
	NARAYEN

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B798	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6H	<0.03A	 2.4K	 0.82	 0.21	 0.05	 3.5D
	0.05 - 0.1	5.8H	<0.03A	 0.77K	 0.64	 0.06	 0.03	 0D
	0.1 - 0.2	6H	<0.03A
	0.2 - 0.3	6.3H	<0.03A	 0.6K	 0.46	 0.02	 0.05	 0D
	0.3 - 0.34	6.3H	<0.03A
	0.34 - 0.47	6.3H	 0.038A	 5.4K	 7.9	 0.38	 0.74	 3.1D
	0.47 - 0.6	6.4H	 0.041A
	0.6 - 0.76	6.6H	 0.057A
	0.76 - 0.9	7.1H	 0.074A
	0.9 - 1.02	7.4H	 0.104A	 4.5K	 7.1	 0.35	 0.95	 0D
	1.02 - 1.2
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.37A	 34B	 250F	 0.092B	 3.42B	1.40	 14	 70C	 15	 9	 6
	0.05 - 0.1	 0.35A	 7B	 120F	 0.025B	 3.52B	1.50	 14	 71C	 20	 5	 3
	0.1 - 0.2	 0.2A	 7B	 0.015B	1.50	 19	 74C	 19	 5	 2
	0.2 - 0.3	 0.14A	 7B	 0.011B	1.60	 25	 79C	 14	 4	 2
	0.3 - 0.34	 0.15A	 0.011B	1.00	 26	 74C	 18	 3	 3
	0.34 - 0.47	 0.21A	 16B	 220F	 0.029B	 2.92B	 35	 42C	 17	 3	 38
	0.47 - 0.6	 0.12A	 0.018B	 29	 43C	 18	 5	 34
	0.6 - 0.76	 14B	 27	 47C	 17	 5	 31
	0.76 - 0.9	1.60	 17
	0.9 - 1.02	 420F	 2.62B	 28	 52C	 17	 8	 25
	1.02 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.34
	0.34 - 0.47
	0.47 - 0.6
	0.6 - 0.76
	0.76 - 0.9
	0.9 - 1.02
	1.02 - 1.2

	Project Name:	NAR
	Project Code:	NAR	Site ID:	B798	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded