Project Name:	Regional
	Project Code:	REG	Site ID:	T119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	8.6KM north east of Laura along old railway line:
	Date Desc.:	04/07/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7767   1:100000	Rainfall:	920
	Northing/Long.:	144.5	Runoff:	Moderately rapid
	Easting/Lat.:	-15.05	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	24 metres
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Magnesic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Panicum species, Heteropogon triticeus
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tetrodonta, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Reddish brown (5YR4/4-Moist); Brown (7.5YR5/4-Dry); ; Sand; Single grain grade of structure; 
	Loose consistence; Gradual change to - 
	A2	0.1 - 0.2 m	Dark red (2.5YR3/6-Moist); Reddish yellow (5YR6/6-Dry); ; Sand; Single grain grade of structure; 
	Loose consistence; Gradual change to - 
	B1	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); Red (2.5YR5/6-Dry); ; Sand; Single grain grade of structure; Firm 
	consistence; Gradual change to - 
	B1	0.3 - 0.5 m	Dark red (2.5YR3/8-Moist); Red (2.5YR4/8-Dry); ; Sand (Heavy); Massive grade of structure; Firm 
	consistence; Gradual change to - 
	B1	0.5 - 0.6 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Firm consistence; Gradual change to - 
	B21	0.6 - 0.7 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Firm consistence; Very few (0 - 2 %), Argillaceous, , Nodules; Gradual change to - 
	B21	0.7 - 0.8 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Sandy clay loam (Heavy); Massive grade of structure; 
	Earthy fabric; Firm consistence; Very few (0 - 2 %), Argillaceous, , Nodules; Gradual change to -
	B21	0.8 - 0.9 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Strong consistence; Few (2 - 10 %), Argillaceous, , Nodules; Gradual change to - 
	B22	0.9 - 1.2 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Light clay; Massive grade of structure; Earthy fabric; 
	Strong consistence; Common (10 - 20 %), Argillaceous, , Nodules; Gradual change to - 
	B22	1.2 - 1.5 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Light clay; Massive grade of structure; Earthy fabric; 
	Strong consistence; Gradual change to - 
	B22	1.5 - 1.8 m	Red (10R4/8-Moist); Red (10R4/8-Dry); , 5YR66, 0-2% ; , 0-2% ; Light clay; Massive grade of 
	structure; Earthy fabric; Very strong consistence; Gradual change to - 
	1.8 - 2.1 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; Very strong consistence; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	2.1 - 2.4 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Clay loam (Heavy); Massive grade of structure; Earthy 
	fabric; Very strong consistence; Gradual change to - 
	2.4 - 2.7 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Firm consistence; Very few (0 - 2 %), Argillaceous, , Nodules; Gradual change to - 
	2.7 - 3 m	Red (10R4/8-Moist); Red (10R4/8-Dry); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Weak consistence; Many (20 - 50 %), Ferruginous, Medium (2 -6 mm), Nodules; Clear 
	change to - 
	3 - 3.3 m	Red (10R4/8-Moist); Red (10R4/8-Dry); , 5YR66, 10-20% , 5-15mm; , 10-20% , 5-15mm; Sandy 
	clay loam; Massive grade of structure; Earthy fabric; Weak consistence; 2-10%, subrounded, 
	Quartz, coarse fragments; Many (20 - 50 %), Ferruginous, , Nodules; Clear change to - 
	3.3 - 3.4 m	Red (10R4/6-Moist); , 5YR66, 10-20% , 15-30mm, Prominent; , 10-20% , 15-30mm, Prominent; 
	Sandy clay loam; Massive grade of structure; Earthy fabric; Very strong consistence; Clear 
	change to - 
	Morphological Notes
	Observation Notes
	LAYERS RENUMBERED 22-9-92                                                                                               
	Site Notes
	LAURA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2A	 0.017A	 1.1B	 1.1	 0.1	 0.08
	0.1 - 0.2	6.3A	 0.011A	 0.64B	 0.68	 0.09	 0.09
	0.2 - 0.3	6.4A	 0.011A	 0.34B	 0.62	 0.09	 0.09
	0.3 - 0.5	6.4A	 0.011A
	0.5 - 0.6	6.5A	 0.014A	 0.14B	 1.2	 0.15	 0.11
	0.6 - 0.7	6.4A	 0.02A
	0.7 - 0.8	6.5A	 0.014A
	0.8 - 0.9	6.4A	 0.014A
	0.9 - 1.2	6.4A	 0.017A
	1.2 - 1.5	6.5A	 0.017A
	1.5 - 1.8	6.4A	 0.014A	 0.1B	 3.1	 0.19	 0.16
	1.8 - 2.1	6.5A	 0.014A	 0.14B	 2.8	 0.18	 0.22
	2.1 - 2.4	6.5A	 0.014A
	2.4 - 2.7	6.4A	 0.017A
	2.7 - 3	6.4A	 0.017A
	3 - 3.3	6.4A	 0.014A
	3.3 - 3.4	6.6A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.59D	 7.3B	 0.004A	 0.04A	 0.04A	 0	 41A	 52	 3	 4
	0.1 - 0.2	 0.29D	 0.003A	 0.03A	 0.05A	 0	 40A	 52	 4	 4
	0.2 - 0.3	 0	 43A	 48	 3	 5
	0.3 - 0.5	 0	 38A	 51	 3	 8
	0.5 - 0.6	 0	 31A	 48	 3	 18
	0.6 - 0.7	 0.011A	 0.21A	 0	 16A	 48	 4	 32
	0.7 - 0.8	 0	 24A	 38	 3	 31
	0.8 - 0.9
	0.9 - 1.2
	1.2 - 1.5	 0.015A	 0.31A	<2	 28A	 26	 3	 48
	1.5 - 1.8	<2	 19A	 26	 3	 52
	1.8 - 2.1	<2	 23A	 29	 3	 45
	2.1 - 2.4
	2.4 - 2.7	 4	 24A	 30	 4	 42
	2.7 - 3
	3 - 3.3	 0.016A	 0.34A	 30	 31A	 28	 7	 34
	3.3 - 3.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.8 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.4

	Project Name:	Regional
	Project Code:	REG	Site ID:	T119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction