Project Name:	Regional
	Project Code:	REG	Site ID:	T153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	23.2KM west of Croydon Pub on Normanton Road:
	Date Desc.:	29/09/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7361   1:100000	Rainfall:	0
	Northing/Long.:	142.083333333333	Runoff:	Very slow
	Easting/Lat.:	-18.0833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pge	Substrate Material:	Undisturbed soil core, 2.4 m deep,No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Mesotrophic Grey Kandosol     	Principal Profile Form:	Gn2.94
	ASC Confidence:	Great Soil Group:	Grey earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Melaleuca viridiflora, Eucalyptus species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Loamy sand; Single grain grade of structure; Moist; Very weak 
	consistence; Few, fine (1-2mm) roots; Clear change to - 
	A11	0.05 - 0.1 m	Dark grey (10YR4/1-Moist); ; Loamy sand; Single grain grade of structure; Moist; Very weak 
	consistence; Few, fine (1-2mm) roots; Clear change to - 
	A21	0.1 - 0.2 m	Light brownish grey (10YR6/2-Moist); Pinkish grey (7.5YR7/2-Dry); ; Sand (Heavy); Massive grade
	 of structure; Dry; Very strong consistence; Common, medium (2-5mm) roots; Gradual change to
	 - 
	A22	0.2 - 0.3 m	Pale brown (10YR6/3-Moist); Pinkish grey (7.5YR7/2-Dry); ; Sand (Heavy); Massive grade of 
	structure; Dry; Very strong consistence; Few, fine (1-2mm) roots; Gradual change to - 
	A23	0.3 - 0.4 m	Pale brown (10YR6/3-Moist); Pinkish grey (7.5YR7/2-Dry); ; Sand (Heavy); Massive grade of 
	structure; Dry; Rigid consistence; Few, fine (1-2mm) roots; Gradual change to - 
	A3	0.4 - 0.5 m	Pale brown (10YR6/3-Moist); , 10YR68, 2-10% ; , 2-10% ; Sandy loam (Heavy); Massive grade of 
	structure; Earthy fabric; Dry; Very strong consistence; Few (2 - 10 %), Manganiferous, Coarse (6 -
	 20 mm), Concretions; FewGradual change to - 
	B1	0.5 - 0.6 m	Brownish yellow (10YR6/5-Moist); , 10YR68, 2-10% , 5-15mm, Prominent; , 2-10% , 5-15mm, 
	Prominent; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 20 mm), Concretions; Gradual change 
	to - 
	B21	0.6 - 0.7 m	Light grey (10YR7/2-Moist); , 10YR68, 2-10% , 5-15mm, Prominent; , 2-10% , 5-15mm, 
	Prominent; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 20 mm), Concretions; Gradual change 
	to - 
	B21	0.7 - 0.8 m	Light grey (10YR7/2-Moist); , 10YR68, 10-20% ; , 10-20% ; Sandy medium clay; Massive grade of
	 structure; Earthy fabric; Dry; Rigid consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 20 
	mm), Concretions; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B21	0.8 - 0.9 m	Light grey (10YR7/2-Moist); , 7.5YR78, 20-50% , 15-30mm, Distinct; , 20-50% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 20 mm), Concretions; Gradual change 
	to - 
	B21	0.9 - 1 m	Light grey (10YR7/2-Moist); , 7.5YR78, 20-50% , 15-30mm, Distinct; , 20-50% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Very few (0 - 2 %), Manganiferous, , Concretions; Gradual change to - 
	B22	1 - 1.1 m	Light grey (10YR7/2-Moist); , 7.5YR78, 10-20% , Distinct; , 10-20% , Distinct; Light medium clay;
	 Massive grade of structure; Earthy fabric; Dry; Very strong consistence; Few (2 - 10 %), 
	Manganiferous, , Concretions; Gradual change to - 
	B22	1.1 - 1.2 m	Light grey (10YR7/2-Moist); , 10YR66; Light medium clay; Massive grade of structure; Earthy 
	fabric; Dry; Strong consistence; Few (2 - 10 %), Manganiferous, , Concretions; Gradual change 
	to - 
	1.2 - 1.35 m	Light grey (10YR7/2-Moist); , 0-2% ; , 0-2% ; Sandy medium clay (Heavy); Massive grade of 
	structure; Earthy fabric; Strong consistence; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), 
	Concretions; Gradual change to - 
	1.35 - 1.5 m	Light grey (2.5Y7/2-Moist); , 0-2% ; , 0-2% ; Sandy medium clay (Heavy); Massive grade of 
	structure; Earthy fabric; Rigid consistence; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), 
	Concretions; Gradual change to - 
	C	1.5 - 1.8 m	Light grey (2.5Y7/2-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Rigid consistence; Common (10 - 20 %), Ferruginous, Very coarse (20 - 60 mm), Concretions; 
	Gradual change to - 
	1.8 - 2.1 m	Light grey (2.5Y7/2-Moist); ; Medium clay; Massive grade of structure; Rigid consistence; Very 
	many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Concretions; Gradual change to - 
	2.1 - 2.2 m	Light grey (2.5Y7/2-Moist); ; Medium heavy clay; Massive grade of structure; Rigid consistence; 
	Many (20 - 50 %), Ferruginous, , Concretions; Gradual change to - 
	2.2 - 2.35 m	Light grey (2.5Y7/2-Moist); ; Medium heavy clay; Massive grade of structure; Rigid consistence; 
	Clear change to - 
	2.35 - 2.45 m	Light grey (2.5Y7/2-Moist); ; Medium heavy clay; Massive grade of structure; Rigid consistence; 
	Morphological Notes
	Observation Notes
	>60CM INCREASING Y MATRIX:40-90CM CONC. INSIDE MOTTLE:180-210CM CONSISTS OF CONC.& COARSE MOTTLES 
	&SANDY LENSES:        
	Site Notes
	CROYDON

	Project Name:	Regional
	Project Code:	REG	Site ID:	T153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.5A	 0.032A	 1.2B	 0.36	 0.1	 0.18	 0.9F	 2.7F
	0.05 - 0.1	6.5A	 0.032A	 0.92B	 0.21	 0.08	 0.2	 0.3F	 1.7F
	0.1 - 0.2	6.7A	 0.017A	 0.66B	 0.15	 0.07	 0.17	 0.5F	 1.6F
	0.2 - 0.3	6.6A	 0.014A	 0.36B	 0.14	 0.08	 0.18	 0.05F	 0.8F
	0.3 - 0.4	6.2A	 0.011A	 0.32B	 0.17	 0.07	 0.17
	0.4 - 0.5	6.2A	 0.017A	 0.46B	 0.29	 0.11	 0.18	 0.5F	 1.5F
	0.5 - 0.6	6A	 0.017A	 0.76B	 0.46	 0.15	 0.18	 0.7F	 2.3F
	0.6 - 0.7	6.2A	 0.017A
	0.7 - 0.8	6.3A	 0.014A	 1B	 0.08	 0.13	 0.18	 0.5F	 1.9F
	0.8 - 0.9	6.5A	 0.017A
	0.9 - 1	6.7A	 0.017A	 1.1B	 1.2	 0.15	 0.18	 0.9F	 3.5F
	1 - 1.1	6.7A	 0.017A
	1.1 - 1.2	6.7A	 0.02A	 1B	 1.67	 0.19	 0.26	 0.5F	 3.18A	 3.6F	8.18
	1.2 - 1.35	6.2A	 0.089A	 0.76B	 1.7	 0.2	 0.42	 1.1F	 4.2F
	1.35 - 1.5	6.8A	 0.026A
	1.5 - 1.8	6.9A	 0.029A	 0.26B	 1.5	 0.22	 0.4
	1.8 - 2.1	6.5A	 0.041A
	2.1 - 2.2	6.1A	 0.044A	 0.26B	 2.7	 0.21	 1.6
	2.2 - 2.35	5.9A	 0.05A
	2.35 - 2.45	6.4A	 0.035A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.43D	 2.8B	 0.005A	 0.03A	 0.43A	 0	 58A	 35	 4	 3
	0.05 - 0.1	 0.12D	<2B	 0.006A	 0.03A	 0.43A	 0	 50A	 43	 4	 3
	0.1 - 0.2	 0.07D	<2B	 0.005A	 0.45A	 0	 52A	 41	 4	 3
	0.2 - 0.3	<2B	 0.005A	 0.47A	 0	 49A	 43	 4	 4
	0.3 - 0.4
	0.4 - 0.5	 0.005A	 0.57A	<2	 47A	 37	 4	 12
	0.5 - 0.6	 2	 45A	 35	 3	 17
	0.6 - 0.7
	0.7 - 0.8	<2B	 0.006A	 0.59A	 2	 45A	 29	 3	 23
	0.8 - 0.9
	0.9 - 1	 2	 48A	 23	 3	 26
	1 - 1.1
	1.1 - 1.2	 2	 46A	 23	 3	 28
	1.2 - 1.35	 0.007A	 0.64A	 2	 49A	 23	 3	 25
	1.35 - 1.5
	1.5 - 1.8	 2	 50A	 24	 3	 23
	1.8 - 2.1
	2.1 - 2.2
	2.2 - 2.35
	2.35 - 2.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05

	Project Name:	Regional
	Project Code:	REG	Site ID:	T153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.35
	1.35 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.2
	2.2 - 2.35
	2.35 - 2.45

	Project Name:	Regional
	Project Code:	REG	Site ID:	T153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction