Project Name:	Regional
	Project Code:	REG	Site ID:	T319	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	I. Lepsch	Locality:
	Date Desc.:	15/09/81	Elevation:	 66 metres
	Map Ref.:	Sheet No. : 8062   1:10000	Rainfall:	3500
	Northing/Long.:	145.958333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-17.65	Drainage:	Well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Lava plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol     	Principal Profile Form:	Uf6.31
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.2 m	Dusky red (10R3/4-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Granular; Moist; 
	Weak consistence; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Diffuse change to - 
	B1	0.2 - 0.5 m	Dark red (10R3/5-Moist); ; Medium clay; Weak grade of structure, 5-10 mm, Subangular blocky; 
	Moist; Weak consistence; Very few (0 - 2 %), Ferromanganiferous, , Nodules; Diffuse change to 
	- 
	B21	0.5 - 1 m	Dark red (10R3/5-Moist); ; Medium clay; Massive grade of structure; Moist; Weak consistence; 
	Very few (0 - 2 %), Ferromanganiferous, , Nodules; Diffuse change to - 
	B22	1 - 1.4 m	Dark red (10R3/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak consistence; 
	Very few (0 - 2 %), Ferromanganiferous, , Nodules; Diffuse change to - 
	B23	1.4 - 1.8 m	Dark red (10R3/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak consistence; 
	Very few (0 - 2 %), Ferromanganiferous, , Nodules; Clear change to - 
	B31	1.8 - 2.2 m	Dark red (10R3/6-Moist); ; Medium clay; Massive grade of structure; Moist; Weak consistence; 
	Diffuse change to - 
	B32	2.2 - 2.5 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Firm consistence; 
	Morphological Notes
	Observation Notes
	SOME TABULAR YELLOW CONCRETIONS FROM 180CM:                                                                             
	Site Notes
	INNISFAIL

	Project Name:	Regional
	Project Code:	REG	Site ID:	T319	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	4.7D	 0.02H	<0.01	 0.05	 0.02	 0.4F	 1.34A	 0.5F	1.49
	5A
	0.2 - 0.5	5D	 0.02H	<0.01	 0.04	 0.02	 0.2F	 0.3F
	5.2A
	0.5 - 1	5.4D	 0.04H	 0.1	 0.05	 0.03	 0.2F	 0.4F
	5.4A
	1 - 1.4	5.5D
	5.4A
	1.4 - 1.8	5.6D	 0.02H	<0.01	 0.04	 0.03	 0.2F	 0.79A	 0.3F	3.80
	5.3A
	1.8 - 2.2	5.7D	 0.06A
	5.4A
	2.2 - 2.5	5.7D	 0.3H	 0.22	 0.08	 0.03	 0.1F	<0.1A	 0.7F
	5.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	 1.45D	 8A	 14	 13	 65
	0.2 - 0.5	 0.83D	 8A	 14	 12	 66
	0.5 - 1	 0.43D	 8A	 15	 10	 67
	1 - 1.4
	1.4 - 1.8	 0.29D	 7A	 13	 13	 67
	1.8 - 2.2
	2.2 - 2.5	 0.03D	 8A	 12	 15	 65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.2 - 0.5
	0.5 - 1
	1 - 1.4
	1.4 - 1.8
	1.8 - 2.2
	2.2 - 2.5

	Project Name:	Regional
	Project Code:	REG	Site ID:	T319	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method