Project Name:	Regional
	Project Code:	REG	Site ID:	TL55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	Webb, Ian	Locality:
	Date Desc.:	15/01/84	Elevation:	No Data
	Map Ref.:	Sheet No. : 7965   1:100000	Rainfall:	0
	Northing/Long.:	145.1	Runoff:	Rapid
	Easting/Lat.:	-16.2833333333333	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	10 % 	Aspect:	350 degrees
	Surface Soil Condition (dry):	N/A
	Erosion:	Partial, Moderate (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Brown (7.5YR4/4-Moist); ; Sandy clay loam; Single grain grade of structure; Very weak 
	consistence; 20-50%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; 
	AbundantSharp, Smooth change to - 
	0.03 - 0.05 m	Strong brown (7.5YR4/6-Moist); ; Clay loam, fine sandy; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Rough-ped fabric; Weak consistence; 10-20%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; ManyAbrupt, Smooth change to - 
	0.05 - 0.1 m	Yellowish red (5YR4/6-Moist); ; Clay loam, fine sandy; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Rough-ped fabric; Weak consistence; 10-20%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; CommonSmooth change to - 
	0.1 - 0.3 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Weak grade of structure, 5-10 mm, Subangular blocky;
	 Earthy fabric; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, dispersed, Quartz, 
	coarse fragments; CommonClear, Smooth change to - 
	0.3 - 0.6 m	Red (2.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Firm consistence; 10-20%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; 
	FewGradual, Smooth change to - 
	0.6 - 0.9 m	Red (2.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 20-50 mm, Angular blocky; 
	Rough-ped fabric; Very firm consistence; 10-20%, fine gravelly, 2-6mm, angular, dispersed, 
	Quartz, coarse fragments; FewDiffuse, Smooth change to - 
	0.9 - 1.8 m	Red (2.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 20-50 mm, Angular blocky; 
	Rough-ped fabric; Very firm consistence; 10-20%, fine gravelly, 2-6mm, angular, dispersed, 
	Quartz, coarse fragments; Gradual, Smooth change to - 
	1.8 - 2.4 m	Red (2.5YR4/8-Moist); ; Light medium clay; Weak grade of structure, 20-50 mm, Angular blocky; 
	10-20%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	WAS ORIGINALLY EP44:M3610-M3618:                                                                                        
	Site Notes
	MT. WINDSOR

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	4D	 1.5H	 2.42	 0.51	 0.24	 1.6F	 4.9J	 6.27B	4.90
	4.4A	 0.78B
	4I	 0.82H
	0.05 - 0.1	4.2D	 0.27H	 0.8	 0.26	 0.14	 0.99F	 3.8J	 2.46B	3.68
	4.4A	 0.58B
	4.2I	 0.41H
	0.1 - 0.2	4.3D	 0.1H	 0.57	 0.16	 0.12	 0.86F	 2.8J	 1.81B	4.29
	4.6A	 0.52B
	4.3I	 0.34H
	0.2 - 0.3	4.5D	 0.1H	 0.24	 0.06	 0.05	 0.55F	 2.5J	 1B	2.00
	4.2A	 0.38B
	4.1I	 0.17H
	0.3 - 0.6	4.54D	 0.08H	 0.17	 0.04	 0.05	 0.72F	 2.3J	 1.06B	2.17
	4.5A	 0.72B
	4.2I	 0H
	0.6 - 0.9	4.4D	 0.07H	 0.15	 0.04	 0.06	 0.82F	 1.7J	 1.14B	3.53
	4.6A	 0.77B
	4.2I	 0.05H
	0.9 - 1.2	4.5A	 0.07H	 0.22	 0.04	 0.06	 0.66F	 1.05B
	4.2I	 0.6B
	 0.06H
	1.2 - 1.5	4.6A	 0.07H	 0.43	 0.03	 0.04	 0.44F	 1.01B
	4.2I	 0.4B
	 0.04H
	1.5 - 1.8	4.6A	 0.07H	 0.55	 0.05	 0.04	 0.4F	 1.11B
	4.2I	 0.34B
	 0.06H
	1.8 - 2.1	4.6A	 0.07H	 0.57	 0.053	 0.04	 0.22F	 0.95B
	4.3I	 0.22B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 10.4D
	0.05 - 0.1	 5.37D
	0.1 - 0.2	 3.86D
	0.2 - 0.3	 2.31D
	0.3 - 0.6	 1.37D
	0.6 - 0.9	 1.03D
	0.9 - 1.2	 0.91D
	1.2 - 1.5	 0.7D
	1.5 - 1.8	 0.55D
	1.8 - 2.1	 0.36D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	TL55	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15G_C_AL1	Exchangeable aluminium - meq per 100g of soil - Aluminium By difference of C and A or B
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method