Project Name:	RR
	Project Code:	RR	Site ID:	B187	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	20/08/53	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 9442   1:100000	Rainfall:	830
	Northing/Long.:	152.720833333333	Runoff:	Moderately rapid
	Easting/Lat.:	-27.8083333333333	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Td	Substrate Material:	Soil pit, 0.3 m deep,Dolomite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	26.2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Petroclcic Leptic Calcarosol     	Principal Profile Form:	Uf6.32
	ASC Confidence:	Great Soil Group:	Rendzina
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus tessellaris, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.15 m	Black (10YR2/1-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Granular; Dry; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, Chert, coarse fragments; Few (2 - 10 %), 
	Calcareous, , ; Field pH 7.9 (pH meter); Gradual change to - 
	B	0.15 - 0.23 m	Black (10YR2/1-Moist); ; Medium clay; Strong grade of structure, Subangular blocky; Strong 
	grade of structure, 2-5 mm, Granular; Dry; Firm consistence; Common (10 - 20 %), Calcareous, , 
	; Field pH 8.1 (pH meter); Gradual change to - 
	C	0.28 - 0.41 m	White (10YR8/1-Moist); , 10YR62; Field pH 8.9 (pH meter); 
	Morphological Notes
	C	Amorphous dolomite
	Observation Notes
	VERTICLE EXPOSURE                                                                                                       
	Site Notes
	IPSWICH

	Project Name:	RR
	Project Code:	RR	Site ID:	B187	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	7.9H	 0.07B
	0.15 - 0.23	8.1H	 0.07B
	0.28 - 0.41	8.9H	 0.05B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 2.46C
	0.15 - 0.23	 20.7C
	0.28 - 0.41	 86.3C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.23
	0.28 - 0.41

	Project Name:	RR
	Project Code:	RR	Site ID:	B187	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede