Project Name:	RR
	Project Code:	RR	Site ID:	B259	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	W.H. Litchfield	Locality:
	Date Desc.:	01/02/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 9149   1:100000	Rainfall:	863
	Northing/Long.:	151.397777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-24.08	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 PRm	Substrate Material:	Soil pit, 1 m deep,Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	18 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Grey Chromosol     	Principal Profile Form:	Dy3.22
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Heteropogon contortus
	Tall Strata - Tree, , Isolated plants. *Species includes - Eucalyptus dichromophloia, Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.15 m	Dark grey (10YR4/1-Moist); ; Sandy clay loam; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Moderately moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, Substrate material, 
	coarse fragments; Field pH 6.4 (pH meter); Many, very fine (0-1mm) roots; Gradual change to - 
	A12	0.15 - 0.23 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam; Weak grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, Substrate 
	material, coarse fragments; Field pH 6.4 (pH meter); Few, very fine (0-1mm) roots; Clear change 
	to - 
	B2	0.23 - 0.51 m	Dark greyish brown (2.5Y4/2-Moist); , 5YR44; Medium clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Very firm consistence; Field pH 7.5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	RODDS BAY

	Project Name:	RR
	Project Code:	RR	Site ID:	B259	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.4H	 0.03B	 10.3K	 6.2	 0.1	 0.12	 5D
	0.15 - 0.23	6.4H	 0.026B
	0.23 - 0.51	7.5H	 0.036B	 16.2K	 7.6	 0.04	 0.51	 0.44D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 1.84A	 17C	 0.03F	 0.11B	 0.4	 26C	 44	 9	 17
	0.15 - 0.23	 0.78A	 0.07B	 1	 29C	 42	 7	 20
	0.23 - 0.51	 0.48A	 0.04B	 0	 19C	 35	 6	 40
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.23
	0.23 - 0.51

	Project Name:	RR
	Project Code:	RR	Site ID:	B259	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded