Project Name:	RR
	Project Code:	RR	Site ID:	B284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	04/10/56	Elevation:	 152 metres
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	4826
	Northing/Long.:	145.805555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-17.8486111111111	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgb	Substrate Material:	Auger boring, 4.5 m deep,Granite 
	Land Form
	Rel/Slope Class: 	Steep mountains >300m 32-	Pattern Type:	Mountains
	56%
	Morph. Type:	Crest	Relief:	61 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	35 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Dermosol     	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Fern, , . *Species includes - Pteridium esculentum
	Mid Strata - Vine, , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - Agathis robusta
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, 
	Granular; Moist; Very weak consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Field 
	pH 5.7 (pH meter); Abundant, fine (1-2mm) roots; Clear change to - 
	B1	0.06 - 0.23 m	Brown (7.5YR4/2-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Polyhedral; Moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Field pH 5.6 (pH meter); 
	Many, fine (1-2mm) roots; Gradual change to - 
	B21	0.23 - 0.64 m	Red (2.5YR4/8-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Polyhedral; Moist; Weak
	 consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	B22	0.64 - 1.12 m	Red (2.5YR4/8-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Polyhedral; Moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	B31	1.12 - 1.83 m	Red (2.5YR5/8-Moist); ; Clay loam; Massive grade of structure; Moist; Weak consistence; 10-
	20%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	B32	2.13 - 2.59 m	Red (2.5YR5/8-Moist); ; Clay loam (Light); Massive grade of structure; Moist; Weak consistence; 
	2-10%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	B33	3.35 - 3.81 m	Red (2.5YR5/8-Moist); ; Loam (Light); Massive grade of structure; Moist; Weak consistence; 2-
	10%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	B33	4.12 - 4.57 m	Red (2.5YR5/8-Moist); ; Loam (Light); Massive grade of structure; Moist; Very weak consistence; 
	20-50%, fine gravelly, 2-6mm, coarse fragments; Diffuse change to - 
	C	4.57 - 4.8 m	; 
	C	4.8 - 5.72 m	; 
	R	 -  m	Rock 
	Morphological Notes
	C	Greenish grey-grey speckled weathered granite

	Project Name:	RR
	Project Code:	RR	Site ID:	B284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	Greenish grey-grey speckled weathered granite
	R	Rock sampled adjacent to site
	Observation Notes
	0-6CM A1 + A2 HORIZON                                                                                                   
	Site Notes
	TULLY

	Project Name:	RR
	Project Code:	RR	Site ID:	B284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.7H
	0.06 - 0.23	5.6H
	0.23 - 0.64
	0.64 - 1.12
	1.12 - 1.83
	2.13 - 2.59
	3.35 - 3.81
	4.12 - 4.57
	4.57 - 4.8
	4.8 - 5.72
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.044F	1.30	 8	 62C	 12	 9	 13
	0.06 - 0.23	 0.031F	1.40	 11	 40C	 13	 14	 29
	0.23 - 0.64	 0.023F	1.40
	0.64 - 1.12	 0.021F	1.50	 5	 16C	 21	 23	 39
	1.12 - 1.83	 0.02F	1.50
	2.13 - 2.59	 0.016F	1.50	 5	 16C	 31	 28	 27
	3.35 - 3.81	 0.019F	1.50
	4.12 - 4.57	 0.02F	1.60	 40	 29C	 33	 27	 16
	4.57 - 4.8	 0.039F	2.40	 10	 61C	 28	 10	 3
	4.8 - 5.72
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.06 - 0.23
	0.23 - 0.64
	0.64 - 1.12
	1.12 - 1.83
	2.13 - 2.59
	3.35 - 3.81
	4.12 - 4.57
	4.57 - 4.8
	4.8 - 5.72
	 - 

	Project Name:	RR
	Project Code:	RR	Site ID:	B284	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	4_NR	pH of soil - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded