Project Name:	RR
	Project Code:	RR	Site ID:	B288	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/10/56	Elevation:	 30 metres
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	0
	Northing/Long.:	145.860555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-17.9041666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, 4 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - Agathis robusta, Eucalyptus delegatensis
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, , Granite
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy clay loam; Strong grade of structure, 2-5 mm, 
	Granular; Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; 
	Field pH 5.4 (pH meter); Many, very fine (0-1mm) roots; Clear change to - 
	A3	0.05 - 0.23 m	Dark red (2.5YR3/6-Moist); ; Clay loam, sandy; Strong grade of structure, 5-10 mm, Angular 
	blocky; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field 
	pH 5.2 (pH meter); Common, very fine (0-1mm) roots; Gradual change to - 
	B2	0.3 - 0.61 m	Red (2.5YR4/8-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Angular blocky; Moist; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.2 (pH 
	meter); Diffuse change to - 
	B2	0.76 - 1.37 m	Red (10R4/6-Moist); ; Light clay; Massive grade of structure; Moist; Weak consistence; 2-10%, 
	fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.4 (pH meter); Diffuse change to - 
	B2	1.52 - 1.88 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Moist; Weak consistence; 2-10%,
	 fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.3 (pH meter); Diffuse change to - 
	B3	2.13 - 2.74 m	Red (2.5YR4/8-Moist); ; Clay loam; Massive grade of structure; Moist; Weak consistence; 10-
	20%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 5.3 (pH meter); Diffuse 
	change to - 
	B3	3.35 - 3.96 m	Red (2.5YR4/6-Moist); ; Clay loam; Massive grade of structure; Moist; Weak consistence; 10-
	20%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 5.2 (pH meter); Diffuse 
	change to - 
	4.57 - 5.18 m	Red (2.5YR4/6-Moist); ; Clay loam; Massive grade of structure; Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.2 (pH meter); Diffuse change to - 
	5.56 - 6.17 m	Red (2.5YR4/8-Moist); ; Clay loam; Massive grade of structure; Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.1 (pH meter); Diffuse change to - 
	7.01 - 7.16 m	Red (2.5YR4/8-Moist); ; Loam; Massive grade of structure; Weak consistence; 10-20%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.1 (pH meter); 
	Morphological Notes

	Project Name:	RR
	Project Code:	RR	Site ID:	B288	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0-5CM POROUS GRANULAR                                                                                                   
	Site Notes
	TULLY
	Observation Notes

	Project Name:	RR
	Project Code:	RR	Site ID:	B288	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.4H	 0.02B
	0.05 - 0.23	5.2H	 0.01B	 0.05K	 0	 0.08	 0.06	 4.9D
	0.3 - 0.61	5.2H	 0.01B	 0.05K	 0	 0.02	 0.04	 2.5D
	0.76 - 1.37	5.4H	 0.01B
	1.52 - 1.88	5.3H	 0.01B	 0.05K	 0	 0.01	 0.03	 1D
	2.13 - 2.74	5.3H	 0.01B
	3.35 - 3.96	5.2H	 0.01B
	4.57 - 5.18	5.2H	 0.01B
	5.56 - 6.17	5.1H	 0.01B
	7.01 - 7.16	5.1H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.02A	 5	 36C	 26	 8	 26
	0.05 - 0.23	 1.59A	 3C	 0.049F	 0.13B	 2	 37C	 24	 5	 32
	0.3 - 0.61	 0.33A
	0.76 - 1.37	 0.18A	 5	 32C	 28	 9	 30
	1.52 - 1.88	 9	 35C	 26	 8	 32
	2.13 - 2.74	 11	 33C	 30	 13	 24
	3.35 - 3.96
	4.57 - 5.18	 7	 28C	 30	 14	 28
	5.56 - 6.17
	7.01 - 7.16	 14	 31C	 30	 16	 21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.23
	0.3 - 0.61
	0.76 - 1.37
	1.52 - 1.88
	2.13 - 2.74
	3.35 - 3.96
	4.57 - 5.18
	5.56 - 6.17
	7.01 - 7.16

	Project Name:	RR
	Project Code:	RR	Site ID:	B288	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded