Project Name:	RR
	Project Code:	RR	Site ID:	B365	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:
	Date Desc.:	16/01/59	Elevation:	 488 metres
	Map Ref.:	Sheet No. : 9245   1:100000	Rainfall:	0
	Northing/Long.:	151.817777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-26.4305555555556	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tm	Substrate Material:	Auger boring, 2.6 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Ridge	Relief:	30 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Uf5
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Chloris gayana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Angular 
	blocky; Moist; Weak consistence; Field pH 6.2 (pH meter); Clear change to - 
	B21	0.08 - 0.3 m	Dark red (2.5YR3/5-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Moist; Weak consistence; Field pH 6.4 (pH meter); Gradual change to - 
	B22	0.3 - 0.6 m	Dark red (2.5YR3/5-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Moist; Weak consistence; Field pH 4.9 (pH meter); Diffuse change to - 
	B23	0.6 - 0.9 m	Dark red (2.5YR3/5-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Moist; Weak consistence; Field pH 4.6 (pH meter); Diffuse change to - 
	B24	0.9 - 1.2 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Angular blocky; Moderately moist; Firm consistence; 
	0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; Field pH 4.7 (pH meter); Diffuse 
	change to - 
	B25	1.2 - 1.85 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Angular blocky; Moderately moist; Firm consistence; 
	0-2%, medium gravelly, 6-20mm, Basalt, coarse fragments; Field pH 4.7 (pH meter); Diffuse 
	change to - 
	BC	1.85 - 2.6 m	Red (2.5YR4/6-Moist); ; Light medium clay; , Angular blocky; Moderately moist; Firm 
	consistence; Field pH 4.5 (pH meter); Clear change to - 
	C	2.6 - 2.7 m	; Field pH 4.5 (pH meter); 
	Morphological Notes
	C	Weathered basalt with pockets of red clay:
	Observation Notes
	Site Notes
	MEMERAMBI

	Project Name:	RR
	Project Code:	RR	Site ID:	B365	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.2H	 0.02C	 8.4K	 2.1	 1.2	 0.31	 26.7J	1.16
	0.08 - 0.3	6.4H	 0.02C
	0.3 - 0.6	4.9H	 0.02C
	0.6 - 0.9	4.6H	 0.02C	 0.24K	 2.6	 0.08	 0.06	 16.1J	0.37
	0.9 - 1.2	4.7H	 0.02C
	1.2 - 1.85	4.7H	 0.02C	<0.1K	 3.7	 0.15	 0.02	 11.8J	0.17
	1.85 - 2.6	4.5H	 0.03C
	2.6 - 2.7	4.5H	 0.04C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 4.12E	 33C	 0.069F	 0.36B	 4C	 11	 18	 61
	0.08 - 0.3	 1.3E	 5C	 0.016F	 4C	 12	 18	 67
	0.3 - 0.6
	0.6 - 0.9	 0.68E	 0.05B	 2C	 7	 12	 81
	0.9 - 1.2
	1.2 - 1.85	 0.04F	 4C	 17	 16	 66
	1.85 - 2.6
	2.6 - 2.7	 1C	 31	 31	 38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.85
	1.85 - 2.6
	2.6 - 2.7

	Project Name:	RR
	Project Code:	RR	Site ID:	B365	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded