Project Name:	RR
	Project Code:	RR	Site ID:	B499	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	10/09/63	Elevation:	 30 metres
	Map Ref.:	Sheet No. : 9346   1:100000	Rainfall:	1092
	Northing/Long.:	152.466666666667	Runoff:	Very slow
	Easting/Lat.:	-25.3166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Te	Substrate Material:	Soil pit, 1.1 m deep,Siltstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Magnesic Mottled-Subnatric Brown Sodosol     	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus punctata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Dry; Very 
	firm consistence; 0-2%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Field pH 
	5.6 (pH meter); Common, fine (1-2mm) roots; Clear change to - 
	A21	0.08 - 0.24 m	Brown (10YR5/3-Moist); ; Fine sandy loam; Massive grade of structure; Moderately moist; Firm 
	consistence; 2-10%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Very few 
	(0 - 2 %), Ferromanganiferous, , Nodules; Field pH 5.7 (pH meter); Few, fine (1-2mm) roots; Clear
	 change to - 
	A22	0.24 - 0.29 m	Light grey (10YR7/2-Moist); ; Fine sandy loam; Massive grade of structure; Many (>5 per 0.01m2) 
	Medium (2-5mm) macropores, Moderately moist; Firm consistence; 20-50%, medium gravelly, 6-
	20mm, Substrate material, coarse fragments; Very few (0 - 2 %), Ferromanganiferous, , Nodules;
	 Field pH 5.9 (pH meter); Few, fine (1-2mm) roots; Abrupt change to - 
	B21	0.29 - 0.51 m	Yellowish brown (10YR5/7-Moist); , 2.5YR47, 20-50% , 5-15mm, Prominent; , 10YR53, 20-50% , 
	5-15mm, Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm
	 consistence; 10-20%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Very few (0 - 
	2 %), Ferromanganiferous, , Nodules; Field pH 6 (pH meter); Few, fine (1-2mm) roots; Gradual 
	change to - 
	B22	0.51 - 0.76 m	Yellowish brown (10YR5/8-Moist); , 2.5YR47, 20-50% , 5-15mm, Prominent; , 10YR62, 20-50% , 
	5-15mm, Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Moist; Firm
	 consistence; 2-10%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Field pH 5.9 
	(pH meter); Gradual change to - 
	B23	0.76 - 1.02 m	Yellowish brown (10YR5/8-Moist); , 10YR61, 20-50% , 15-30mm, Prominent; , N60, 20-50% , 15-
	30mm, Prominent; Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; Moist; Firm 
	consistence; 10-20%, medium gravelly, 6-20mm, Substrate material, coarse fragments; Field 
	pH 5.5 (pH meter); 
	Morphological Notes
	Observation Notes
	FINE OCHROUS ROOT TRACINGS AND PATCHES THROUGH A HORIZONS:GLEY FEATURES:                                                

	Project Name:	RR
	Project Code:	RR	Site ID:	B499	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	HOWARD

	Project Name:	RR
	Project Code:	RR	Site ID:	B499	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.6H	 0.01B	 1K	 0.91	0.06	 0.14	 6.3D
	0.08 - 0.24	5.7H	 0.01B
	0.24 - 0.29	5.9H	 0.01B
	0.29 - 0.51	6H	 0.01B	 0.05K	 2.4	 0.02	 0.54	 8.2D
	0.51 - 0.76	5.9H	 0.02B
	0.76 - 1.02	5.5H	 0.02B	<0.02K	 5.5	 0.04	 1.6	 9.8D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.3A	 1C	 0.006F	 0.081B	1.40	 1	 4C	 57	 28	 10
	0.08 - 0.24	 0.63A	 0.006F	 0.048B	1.60	 11	 9C	 52	 25	 12
	0.24 - 0.29	 0.42A	 0.039B	1.80	 46	 21C	 39	 25	 16
	0.29 - 0.51	 0.26A	 0.009F	 0.033B	1.70	 12	 9C	 32	 20	 39
	0.51 - 0.76	 0.15A	 6	 4C	 29	 20	 48
	0.76 - 1.02	 0.13A	 0.008F	 14	 5C	 26	 18	 51
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08	 0.3C	 0.08C
	0.08 - 0.24	 0.26C	 0.08C
	0.24 - 0.29	 0.25C	 0.11C
	0.29 - 0.51	 0.29C	 0.23C
	0.51 - 0.76
	0.76 - 1.02

	Project Name:	RR
	Project Code:	RR	Site ID:	B499	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate