Project Name:	RR
	Project Code:	RR	Site ID:	B552	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	02/09/66	Elevation:	 335 metres
	Map Ref.:	Sheet No. : 9143   1:100000	Rainfall:	635
	Northing/Long.:	151.216666666667	Runoff:	Slow
	Easting/Lat.:	-27.15	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	Undisturbed soil core, 2 m 
	deep,Unconsolidated material 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous-Endohypersodic Crusty Grey Vertosol     	Principal Profile Form:	Ug5.4
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , Sparse. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus populnea
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.01 m	Dark grey (10YR4/1-Moist); ; Light medium clay; Massive grade of structure; Moderately moist; 
	Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Sharp change to - 
	A12	0.01 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 mm, 
	Angular blocky; Moist; Slightly plastic; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; 
	Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Clear change to - 
	A13	0.1 - 0.2 m	Dark grey (10YR4/1-Moist); ; Heavy clay; Strong grade of structure, 50-100 mm, Angular blocky; 
	Moist; Moderately plastic; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Nodules; 
	A13	0.2 - 0.3 m	Dark grey (10YR4/1-Moist); ; Heavy clay; Strong grade of structure, 50-100 mm, Angular blocky; 
	Moist; Moderately plastic; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Nodules; 
	B2	0.3 - 0.41 m	Dark grey (10YR4/1-Moist); ; Heavy clay; , Lenticular; Strong grade of structure, Angular blocky; 
	Moist; Moderately plastic; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Nodules; Clear change to - 
	B2	0.41 - 0.61 m	Dark grey (10YR4/1-Moist); ; Medium heavy clay; , Lenticular; Strong grade of structure, Angular 
	blocky; Moist; Very firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very 
	few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, Fine (0 - 
	2 mm), Nodules; Very few (0 - 2 %), Gypseous, Fine (0 - 2 mm), Nodules; 
	B2	0.61 - 0.91 m	Dark grey (10YR4/1-Moist); ; Heavy clay; , Lenticular; Strong grade of structure, Lenticular; Moist;
	 Very firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), 
	Nodules; Very few (0 - 2 %), Gypseous, Medium (2 -6 mm), Nodules; Diffuse change to - 
	B2	0.91 - 1.22 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Strong grade of structure, Lenticular; Moist; Firm 
	consistence; 2-10%, Quartz, coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 
	mm), Nodules; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Very few (0 - 2 %), 
	Gypseous, Medium (2 -6 mm), Nodules; 

	Project Name:	RR
	Project Code:	RR	Site ID:	B552	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	1.22 - 1.52 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Strong grade of structure, Lenticular; Moist; Firm 
	consistence; 2-10%, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated;
	 Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Very few (0 - 2 %), Gypseous, 
	Medium (2 -6 mm), Nodules; 
	B2	1.52 - 1.83 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Strong grade of structure, Lenticular; Moist; Firm 
	consistence; 0-2%, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated; 
	Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Very few (0 - 2 %), Gypseous, 
	Medium (2 -6 mm), Nodules; 
	B2	1.83 - 2.13 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Strong grade of structure, Lenticular; Moist; Firm 
	consistence; Few cutans, <10% of ped faces or walls coated; Diffuse change to - 
	B2	2.13 - 2.44 m	Grey (10YR5/1-Moist); , 7.5YR54, 20-50% , 5-15mm, Prominent; , 20-50% , 5-15mm, Prominent; 
	Heavy clay; Strong grade of structure, Lenticular; Moist; Firm consistence; Few cutans, <10% of 
	ped faces or walls coated; 
	Morphological Notes
	Observation Notes
	Site Notes
	DALBY

	Project Name:	RR
	Project Code:	RR	Site ID:	B552	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	6.6H	 0.027B	 7.3K	 7.1	 0.58	 0.56	 3.1D
	0.01 - 0.1	7.3H	 0.028B	 11.6K	 8.3	 0.61	 0.56	 3.3D
	0.1 - 0.2	7.6H	 0.081B	 13.1K	 10.1	 0.33	 1.5	 4.8D
	0.2 - 0.3	6.7H	 0.158B
	0.3 - 0.41	7.6H	 0.233B	 15.7K	 16.8	 0.24	 4.2	 2D
	0.41 - 0.61	8.4H	 0.245B
	0.61 - 0.91	8.4H	 0.26B	 12.6K	 14.8	 0.23	 3.8	 0.52D
	0.91 - 1.22	8.7H	 0.28B	 14.7K	 17.9	 0.3	 4.3	 2D
	1.22 - 1.52	8.6H	 0.26B
	1.52 - 1.83	8.5H	 0.26B
	1.83 - 2.13	8H	 0.27B	 14.8K	 20.9	 0.35	 7	 0.41D
	2.13 - 2.44	7.7H	 0.22B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	 1.5A	 56B	 0.026F	 0.13B	<1	 22C	 43	 11	 22
	0.01 - 0.1	 0.85A	 17B	 0.016F	 0.06B	<1	 21C	 31	 14	 32
	0.1 - 0.2	 0.38A	 0.01F	 0.2B	<1	 18C	 28	 14	 40
	0.2 - 0.3
	0.3 - 0.41	 0.46A	 0.015F	 0.2B	<1	 14C	 21	 12	 51
	0.41 - 0.61
	0.61 - 0.91	 1.1C	 0.14A	 0.014F	 0.22B	<1	 18C	 27	 13	 41
	0.91 - 1.22	 0.8C	 0.09A	 0.017F	 0.28B	 3	 13C	 21	 14	 51
	1.22 - 1.52
	1.52 - 1.83
	1.83 - 2.13	 0.4C	 0.06A	 0.019F	 0.34B	<1	 12C	 20	 15	 53
	2.13 - 2.44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.41
	0.41 - 0.61
	0.61 - 0.91
	0.91 - 1.22
	1.22 - 1.52
	1.52 - 1.83
	1.83 - 2.13
	2.13 - 2.44

	Project Name:	RR
	Project Code:	RR	Site ID:	B552	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded