Project Name:	SAM
	Project Code:	SAM	Site ID:	B419	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:	Paddock 6A.
	Date Desc.:	21/12/59	Elevation:	 55 metres
	Map Ref.:	Sheet No. : 9443   1:100000	Rainfall:	1016
	Northing/Long.:	152.883333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-27.3622222222222	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rga	Substrate Material:	Soil pit, 0.76 m deep,Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8.7 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Grey Chromosol     	Principal Profile Form:	Dy3.12
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.16 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam (Heavy); Weak grade of structure, 50-100 
	mm, Prismatic; Moderate grade of structure, 5-10 mm, Angular blocky; Moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.8 (pH meter); 
	AbundantClear change to - 
	B2	0.18 - 0.38 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR56, 2-10% , 0-5mm, Distinct; , 2.5YR48, 2-10% , 0-
	5mm, Distinct; Medium heavy clay; Weak grade of structure, 50-100 mm, Prismatic; Strong 
	grade of structure, 10-20 mm, Angular blocky; Moist; Slightly plastic; Normal plasticity; Field pH 
	5.9 (pH meter); Gradual change to - 
	B3	0.38 - 0.53 m	Grey (2.5Y5/1-Moist); , 7.5YR54, 10-20% , 5-15mm, Distinct; , 2.5YR48, 10-20% , 5-15mm, 
	Distinct; Medium clay; Weak grade of structure, 50-100 mm, Prismatic; Moderate grade of 
	structure, 10-20 mm, Angular blocky; Wet; Moderately plastic; Normal plasticity; Field pH 6.5 
	(pH meter); Gradual change to - 
	BC	0.53 - 0.71 m	Light grey (2.5Y7/1-Moist); , 10YR68, 10-20% , 0-5mm, Distinct; , 10YR81, 10-20% , 0-5mm, 
	Distinct; Sandy medium clay (Heavy); Weak grade of structure, 20-50 mm, Angular blocky; Wet; 
	Moderately plastic; Normal plasticity; Field pH 6.8 (pH meter); Diffuse change to - 
	C1	0.76 - 0.94 m	; Sandy clay loam (Light); Massive grade of structure; Field pH 7.1 (pH meter); Diffuse change to
	 - 
	C2	1.55 - 1.9 m	; Clayey sand; Massive grade of structure; Field pH 7.9 (pH meter); 
	Morphological Notes
	C2	Speckled weathered granodiorite.
	Observation Notes
	38-71CM MANY WEATHERING MINERALS. DARK GREY BROWN SANDY CLAY LOAM FILL BETWEEN PRISM FACES. 76-
	94CM AS FOR 115-190CM.   
	Site Notes
	SAMFORD WEST

	Project Name:	SAM
	Project Code:	SAM	Site ID:	B419	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	5.8H	 0.01B	 3.9K	 1.6	 0.1	 0.08	 3.9D
	0.18 - 0.38	5.9H	 0.02B	 6.6K	 6.1	 0.06	 0.47	 5.5D
	0.38 - 0.53	6.5H	 0.02B
	0.53 - 0.71	6.8H	 0.02B
	0.76 - 0.94	7.1H	 0.02B
	1.55 - 1.9	7.9H	 0.01B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	 1.1A	 0.02F	 0.1B	 0	 32C	 41	 8	 12
	0.18 - 0.38	 0.8A	 0.02F	 0.08B	 0	 21C	 23	 8	 47
	0.38 - 0.53
	0.53 - 0.71
	0.76 - 0.94
	1.55 - 1.9	 0.04F
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.16
	0.18 - 0.38
	0.38 - 0.53
	0.53 - 0.71
	0.76 - 0.94
	1.55 - 1.9

	Project Name:	SAM
	Project Code:	SAM	Site ID:	B419	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded