Project Name:	WQA
	Project Code:	WQA	Site ID:	B589	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 90 metres
	Map Ref.:	Sheet No. : 6649   1:100000	Rainfall:	203
	Northing/Long.:	138.9375	Runoff:	Slow
	Easting/Lat.:	-24.0375	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 1.4 m deep,Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Gypsic Crusty Brown Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Forb, <0.25m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, rounded, Gravel
	Profile Morphology
	A1	0 - 0.1 m	Light yellowish brown (10YR6/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, 
	Polyhedral; Dry; Loose consistence; Very few (0 - 2 %), Calcareous, , Nodules; Gradual 
	change to - 
	B2	0.1 - 0.2 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, , Nodules; 
	B2	0.2 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, , Nodules; 
	B2	0.3 - 0.6 m	Yellowish brown (10YR5/4-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, , Nodules; 
	B2	0.6 - 0.75 m	Yellowish brown (10YR5/4-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Dry; Strong consistence; Very few (0 - 2 %), Calcareous, , Nodules; Very few 
	(0 - 2 %), Gypseous, , Crystals; 
	B2	0.75 - 0.9 m	Yellowish brown (10YR5/4-Moist); ; Heavy clay; Moderate grade of structure, Angular blocky; 
	Dry; Strong consistence; Very few (0 - 2 %), Calcareous, , Nodules; Very few (0 - 2 %), 
	Gypseous, , Crystals; 
	B2	0.9 - 1.2 m	Yellowish brown (10YR5/4-Moist); ; Heavy clay; Moderate grade of structure, Angular blocky; 
	Dry; Strong consistence; Very few (0 - 2 %), Calcareous, , Nodules; Common (10 - 20 %), 
	Gypseous, , Crystals; 
	B2	1.2 - 1.4 m	Yellowish brown (10YR5/4-Moist); , 10YR72, 0-2% ; , 0-2% ; Heavy clay; Dry; Very firm 
	consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Nodules; Many (20 - 50 
	%), Gypseous, , Crystals; Gradual change to - 
	C	1.4 - 1.5 m	Light yellowish brown (10YR6/4-Dry); , 10YR43, 20-50% , 0-5mm, Distinct; , 10YR32, 20-50% , 
	0-5mm, Distinct; Heavy clay; Few (2 - 10 %), Gypseous, , Crystals; 
	1.5 - 1.8 m	Brownish yellow (10YR6/5-Dry); , 10YR72, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Heavy clay; Few (2 - 10 %), Gypseous, , Crystals; 
	1.8 - 2 m	Brownish yellow (10YR6/5-Dry); , 2.5Y62, 20-50% , 5-15mm, Prominent; , 10YR66, 20-50% , 5-
	15mm, Prominent; Heavy clay; Very few (0 - 2 %), Gypseous, , Crystals; 

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B589	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Morphological Notes
	Observation Notes
	140-200CM CLAY WITH SANDY BANDS. VEGETATION FORBLAND.                                                                   
	Site Notes
	SANDRINGHAM

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B589	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.4H	 0.041B	 16.8K	 1.1	 1.3	 0D
	0.1 - 0.2	8.8H	 0.06B
	0.2 - 0.3	8.9H	 0.092B
	0.3 - 0.6	8.5H	 0.49B
	0.6 - 0.75	8.3H	 1.22B
	0.75 - 0.9	7.9H	 3.46B
	0.9 - 1.2	7.8H	 17B
	1.2 - 1.4	7.4H	 34.8B	 10.4
	1.4 - 1.5	7.3H	 7.1B
	1.5 - 1.8	7.2H	 8.5B
	1.8 - 2	7.1H	 9.6B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.42C	 0.18E	 32B	 0.03F	 0.025B	 1.15B	 10C	 42	 5	 41
	0.1 - 0.2	 0.56C
	0.2 - 0.3	 0.59C	 0.16E	 37B	 0.031F	 0.021B	 1.2B	 9C	 40	 9	 39
	0.3 - 0.6	 0.96C	 0.025F	 0.021B	 0.94B
	0.6 - 0.75	 0.98C
	0.75 - 0.9	 0.73C
	0.9 - 1.2	 0.06C	 0.03E	 0.034F	 0.011B	 0.97B	 9C	 28	 4	 43
	1.2 - 1.4	 0C
	1.4 - 1.5	 0.01C
	1.5 - 1.8	 0.02C
	1.8 - 2	 0C	 0.02E	 119B	 0.057F	 0.14B	 1.45B	 8C	 10	 19	 51
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.4
	1.4 - 1.5
	1.5 - 1.8
	1.8 - 2

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B589	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded