Project Name:	WQA
	Project Code:	WQA	Site ID:	B592	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 93 metres
	Map Ref.:	Sheet No. : 6749   1:100000	Rainfall:	203
	Northing/Long.:	139.325	Runoff:	Slow
	Easting/Lat.:	-24.2166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 2 m deep,Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Crusty Red Vertosol     	Principal Profile Form:	Ug5.35
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Forb, <0.25m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, rounded, Gravel
	Profile Morphology
	A1	0 - 0.1 m	Yellowish red (5YR5/5-Moist); Reddish yellow (5YR6/5-Dry); ; Light medium clay; Strong grade 
	of structure, 2-5 mm, Angular blocky; Dry; Loose consistence; Very few (0 - 2 %), Calcareous,
	 Medium (2 -6 mm), Nodules; Clear change to - 
	B2	0.1 - 0.2 m	Reddish brown (5YR5/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular
	 blocky; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, , Nodules; Gradual 
	change to - 
	B2	0.2 - 0.3 m	Reddish brown (5YR5/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular
	 blocky; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, , Nodules; Gradual 
	change to - 
	B2	0.3 - 0.6 m	Strong brown (7.5YR5/5-Moist); Reddish yellow (7.5YR6/5-Dry); ; Medium heavy clay; 
	Moderate grade of structure, Lenticular; Dry; Very firm consistence; Very few (0 - 2 %), 
	Calcareous, , Nodules; Gradual change to - 
	B2	0.6 - 0.9 m	Strong brown (7.5YR5/5-Moist); ; Medium heavy clay; , Lenticular; Dry; Very firm consistence; 
	Very few (0 - 2 %), Calcareous, , Nodules; Gradual change to - 
	B2	0.9 - 1.08 m	Strong brown (7.5YR5/5-Moist); ; Medium heavy clay; , Lenticular; Dry; Very firm consistence; 
	Very few (0 - 2 %), Calcareous, , Nodules; Gradual change to - 
	B2	1.08 - 1.2 m	Strong brown (7.5YR5/8-Moist); , 10YR72, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Medium heavy clay; , Lenticular; Dry; Very firm consistence; Very few (0 - 2 %), 
	Calcareous, , Nodules; Very few (0 - 2 %), Gypseous, , Crystals; Gradual change to - 
	B2	1.2 - 1.5 m	Pale yellow (2.5Y7/3-Moist); , 7.5YR56, 20-50% , 5-15mm, Distinct; , 2.5YR66, 20-50% , 5-
	15mm, Distinct; Medium heavy clay; , Lenticular; Dry; Very firm consistence; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Soft segregations; Few (2 - 10 %), Calcareous, , Nodules; 
	Few (2 - 10 %), Gypseous, , Crystals; Diffuse change to - 
	B2	1.5 - 1.8 m	Pale yellow (2.5Y7/3-Moist); , 7.5YR56, 20-50% , 5-15mm, Distinct; , 2.5YR66, 20-50% , 5-
	15mm, Distinct; Medium heavy clay; , Lenticular; Dry; Very firm consistence; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Soft segregations; Very few (0 - 2 %), Calcareous, , 
	Nodules; Few (2 - 10 %), Gypseous, , Crystals; Diffuse change to - 

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B592	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	1.8 - 2 m	Pale yellow (2.5Y7/3-Moist); , 7.5YR56, 20-50% , 5-15mm, Distinct; , 2.5YR66, 20-50% , 5-
	15mm, Distinct; Medium heavy clay; , Lenticular; Dry; Very firm consistence; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Soft segregations; Very few (0 - 2 %), Calcareous, , 
	Nodules; Few (2 - 10 %), Gypseous, , Crystals; 
	Morphological Notes
	Observation Notes
	PLAIN WITH CLAYPANS BETWEEN VEGETATED SAND RIDGES:FRAGILE SURFACE CRUST1-2MM THICK WITH PEDS 
	CEMENTED IN UNDER SURFACE: SELF-MULCHED, LOOSE BENEATH:
	Site Notes
	BEDOURIE

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B592	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8H	 0.03B	 10.7K	 6.3	 1.1	 0.38	 2.4D
	0.1 - 0.2	8.9H	 0.05B
	0.2 - 0.3	9.2H	 0.06B	 15.1K	 7.3	 0.55	 1.54	 0D
	0.3 - 0.6	9H	 0.19B	 12.1K	 7	 0.5	 3	 0D
	0.6 - 0.9	8.7H	 0.61B
	0.9 - 1.08	8.5H	 1.2B
	1.08 - 1.2	8H	 3B	 15.7K	 7.3	 0.63	 9.1	 0D
	1.2 - 1.5	8H	 5.4B
	1.5 - 1.8	8H	 3.6B	 14.6K	 7.4	 0.59	 9.3	 0D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.03C	 0.13E	 23B	 0.023F	 0.018B	 0.93B	 15C	 49	 5	 30
	0.1 - 0.2	 0.82C
	0.2 - 0.3	 0.98C	 0.09E	 32B	 0.015B	 15C	 49	 6	 28
	0.3 - 0.6	 1C	 0.09E	 0.017F	 0.062B	 0.74B
	0.6 - 0.9	 1C
	0.9 - 1.08	 1.3C
	1.08 - 1.2	 2.8C	 11C	 38	 1	 42
	1.2 - 1.5	 2C
	1.5 - 1.8	 2.4C	 8C	 41	 3	 40
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.08
	1.08 - 1.2
	1.2 - 1.5
	1.5 - 1.8

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B592	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction