Project Name:	WQA
	Project Code:	WQA	Site ID:	B598	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 87 metres
	Map Ref.:	Sheet No. : 6848   1:100000	Rainfall:	203
	Northing/Long.:	139.688888888889	Runoff:	Rapid
	Easting/Lat.:	-24.5055555555556	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Kw	Substrate Material:	Auger boring, 1 m deep,No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Pedaric Red Sodosol     	Principal Profile Form:	Dr1.33
	ASC Confidence:	Great Soil Group:	Desert loam
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	90-100%, medium gravelly, 6-20mm, , Gravel
	Profile Morphology
	A1	0 - 0.04 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Fine sandy loam; Massive grade of structure; 
	Dry; Weak consistence; 50-90%, medium gravelly, 6-20mm, Substrate material, coarse 
	fragments; Sharp change to - 
	B21	0.04 - 0.1 m	Yellowish red (5YR5/5-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Dry; Very weak consistence; Moderately plastic; Subplastic; 0-2%, medium gravelly,
	 6-20mm, Substrate material, coarse fragments; 
	B21	0.1 - 0.2 m	Yellowish red (5YR5/5-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Dry; Very weak consistence; Moderately plastic; Subplastic; 
	B21	0.2 - 0.3 m	Yellowish red (5YR5/5-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Polyhedral; Dry; Very weak consistence; Moderately plastic; Subplastic; Gradual change to - 
	B22	0.3 - 0.5 m	Reddish yellow (7.5YR6/6-Dry); ; Light medium clay; Moderate grade of structure, Polyhedral; 
	Dry; Very weak consistence; Moderately plastic; Subplastic; 
	B22	0.5 - 0.6 m	Brownish yellow (10YR6/6-Dry); ; Light medium clay; Moderate grade of structure, Polyhedral; 
	Dry; Very weak consistence; Moderately plastic; Subplastic; Very few (0 - 2 %), Gypseous, , 
	Crystals; 
	B22	0.6 - 0.75 m	Brownish yellow (10YR6/6-Dry); ; Light medium clay; Moderate grade of structure, Polyhedral; 
	Dry; Weak consistence; Moderately plastic; Subplastic; Very few (0 - 2 %), Gypseous, , 
	Crystals; Gradual change to - 
	C	0.75 - 0.9 m	Yellowish brown (10YR5/6-Dry); , 10YR81, 20-50% , 5-15mm, Distinct; , 10YR66, 20-50% , 5-
	15mm, Distinct; Silty light clay; Massive grade of structure; Dry; Weak consistence; Moderately 
	plastic; Subplastic; Common (10 - 20 %), Gypseous, , Crystals; 
	0.9 - 1.2 m	Yellowish brown (10YR5/6-Dry); , 10YR81, 20-50% , 5-15mm, Distinct; , 10YR66, 20-50% , 5-
	15mm, Distinct; Silty medium clay; Massive grade of structure; Weak consistence; Few (2 - 10 
	%), Gypseous, , Crystals; 
	1.2 - 1.5 m	Yellowish brown (10YR5/6-Dry); , 10YR81, 20-50% , 5-15mm, Distinct; , 10YR66, 20-50% , 5-
	15mm, Distinct; Silty medium clay; Massive grade of structure; Weak consistence; Few (2 - 10 
	%), Gypseous, , Crystals; 
	Morphological Notes
	Observation Notes

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B598	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	NO VEGETATION OCCURS AT SITE:PATCHES OF BLEACH AT BASE OF A1 HORIZON:BELOW 75CM MATERIAL LOOKS LIKE 
	WEATHERED SILTY     MUDSTONE:
	Site Notes
	CLUNY

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B598	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	7.6H	 0.023B	 3K	 1.6	 0.41	 0.95	 2.4D
	0.03 - 0.1	7.5H	 0.38B
	0.1 - 0.2	7.6H	 0.84B
	0.2 - 0.3	7.4H	 1.3B	 10.2K	 6.8	 0.6	 6.8	 0D
	0.3 - 0.5	7.2H	 2.1B
	0.5 - 0.6	7.4H	 5.4B
	0.6 - 0.75	7.6H	 5.4B
	0.75 - 0.9	7.8H	 14B
	0.9 - 1.2	7.7H	 10B
	1.2 - 1.5	7.7H	 7.2B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.06E	 23B	 0.027F	 0.013B	 0.54B	 17C	 65	 9	 10
	0.03 - 0.1	 0.13E	 43B	 0.037F	 0.019B	 0.88B	 10C	 44	 5	 40
	0.1 - 0.2	 0.1E	 0.031F	 0.026B	 0.75B	 9C	 46	 6	 37
	0.2 - 0.3	 0.08E	 51B	 0.032F	 0.016B	 0.71B	 9C	 46	 6	 37
	0.3 - 0.5	 0.11E	 0.037F	 0.019B	 0.72B	 7C	 41	 6	 44
	0.5 - 0.6	 0.04E	 0.042F	 0.011B	 0.68B	 5C	 33	 11	 45
	0.6 - 0.75	 0.04E	 0.038F	 0.014B	 0.67B	 5C	 29	 15	 45
	0.75 - 0.9	 0.04C	 0.03E	 60B	 0.03F	 0.022B	 0.5B
	0.9 - 1.2	 0.02E	 5B	 0.023F	 0.017B	 0.57B
	1.2 - 1.5	 0.02E	 0.021F	 0.014B	 0.59B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B598	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction