Project Name:	WQA
	Project Code:	WQA	Site ID:	B606	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/09/69	Elevation:	 90 metres
	Map Ref.:	Sheet No. : 6948   	Rainfall:	221
	Northing/Long.:	140.469444444444	Runoff:	No Data
	Easting/Lat.:	-24.7472222222222	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Kw	Substrate Material:	Auger boring, 0.2 m deep,Mudstone 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr1.42
	ASC Confidence:	Great Soil Group:	Desert loam
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	90-100%, medium gravelly, 6-20mm, , Gravel
	Profile Morphology
	A1	0 - 0.1 m	Yellowish red (5YR4/6-Moist); Yellowish red (5YR5/6-Dry); ; Loam; Massive grade of structure;
	 Dry; Weak consistence; 50-90%, coarse gravelly, 20-60mm, Gravel, coarse fragments; Field 
	pH 7.1 (pH meter); Abrupt change to - 
	B2	0.1 - 0.2 m	Red (2.5YR4/6-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Angular blocky; Dry; 
	Very firm consistence; Field pH 7 (pH meter); Gradual change to - 
	C	0.2 - 0.3 m	; Field pH 7.5 (pH meter); 
	Morphological Notes
	C	Mottled weathered mudstone.
	Observation Notes
	NO VEGETATION AT SITE: 0-10CM A1 + BLEACHED A2 HORIZON.                                                                 
	Site Notes
	MONKIRA

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B606	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.1H	 0.059B
	0.1 - 0.2	7H	 0.68B
	0.2 - 0.3	7.5H	 0.68B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.11A	 23B	 0.024F	 0.013B	 0.55B	 11C	 65	 11	 13
	0.1 - 0.2	 0.18A	 0.025F	 0.033B	 0.85B	 9C	 12	 8	 70
	0.2 - 0.3	 0.06C	 0.07A	<1B	 0.026B	 54C	 16	 12	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	WQA
	Project Code:	WQA	Site ID:	B606	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction