Project Name:	WQR
	Project Code:	WQR	Site ID:	B425	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	Edye, Les	Locality:
	Date Desc.:	24/08/53	Elevation:	 165 metres
	Map Ref.:	Sheet No. : 7549   1:100000	Rainfall:	356
	Northing/Long.:	143.291666666667	Runoff:	Very slow
	Easting/Lat.:	-24.3416666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Yellow Vertosol     	Principal Profile Form:	Ug5.5
	ASC Confidence:	Great Soil Group:	Brown clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Chenopod shrub, 0.51-1m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (10YR5/3-Dry); ; Light medium clay; , Angular blocky; Dry; Very firm consistence; Field 
	pH 7 (pH meter); Clear change to - 
	B2	0.08 - 0.25 m	Pale brown (10YR6/3-Dry); ; Heavy clay; , Angular blocky; Dry; Strong consistence; Field pH 
	8.1 (pH meter); Gradual change to - 
	B2	0.25 - 0.48 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; , Angular blocky; Moist; Firm consistence;
	 Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 8.5 (pH meter); Gradual change 
	B2	0.48 - 0.74 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; , Lenticular; Moist; Firm consistence; Field
	 pH 7.2 (pH meter); Diffuse change to - 
	B2	0.74 - 1.14 m	Pale brown (10YR6/3-Moist); ; Heavy clay; , Lenticular; Moist; Firm consistence; Very few (0 - 
	2 %), Gypseous, , Crystals; Field pH 7.7 (pH meter); Diffuse change to - 
	B2	1.14 - 1.27 m	Pale brown (10YR6/3-Moist); ; Heavy clay; , Lenticular; Moist; Weak consistence; Very few (0 -
	 2 %), Gypseous, , Crystals; Field pH 7.6 (pH meter); Diffuse change to - 
	B2	1.27 - 1.42 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; , Lenticular; Moist; Weak consistence; 
	Very few (0 - 2 %), Calcareous, , Concretions; Very few (0 - 2 %), Gypseous, , Crystals; Field 
	pH 7.7 (pH meter); Diffuse change to - 
	B2	1.8 - 2.06 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; , Lenticular; Moist; Weak consistence; 
	Very few (0 - 2 %), Gypseous, , Crystals; Field pH 7.8 (pH meter); 
	Morphological Notes
	Observation Notes
	SURFACE CRUST CRACKS INTO HEXAGONAL PLATES TO 75MM WIDTH:MAJOR CRACKS 25-75MM WIDE AND UP TO 70CM 
	APART:                
	Site Notes
	STONEHEDGE

	Project Name:	WQR
	Project Code:	WQR	Site ID:	B425	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7H	 0.59B
	0.08 - 0.25	8.1H	 0.04B
	0.25 - 0.48	8.5H	 0.11B
	0.48 - 0.74	7.2H	 0.72B
	0.74 - 1.14	7.7H	 0.63B
	1.14 - 1.27	7.6H	 1.39B
	1.27 - 1.42	7.7H	 1.41B
	1.8 - 2.06	7.8H	 0.66B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 125C	 0.04F
	0.08 - 0.25
	0.25 - 0.48
	0.48 - 0.74
	0.74 - 1.14
	1.14 - 1.27
	1.27 - 1.42	 0.04F
	1.8 - 2.06
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.25
	0.25 - 0.48
	0.48 - 0.74
	0.74 - 1.14
	1.14 - 1.27
	1.27 - 1.42
	1.8 - 2.06

	Project Name:	WQR
	Project Code:	WQR	Site ID:	B425	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded