Project Name:	WQR
	Project Code:	WQR	Site ID:	B430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	Edye, Les	Locality:
	Date Desc.:	01/08/53	Elevation:	 61 metres
	Map Ref.:	Sheet No. : 6846   1:100000	Rainfall:	147
	Northing/Long.:	139.991666666667	Runoff:	Slow
	Easting/Lat.:	-25.6541666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol     	Principal Profile Form:	Db0.22
	ASC Confidence:	Great Soil Group:	Desert loam
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Sporobolus actinocladus
	Surface Coarse Fragments:	90-100%, medium gravelly, 6-20mm, , Detrital sedimentary rock (unidentified)
	Profile Morphology
	A1	0 - 0.05 m	Pink (7.5YR7/4-Dry); ; Sandy loam; Massive grade of structure; Dry; Weak consistence; 50-
	90%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Field pH 6.7 (pH meter); 
	Clear change to - 
	A2	0.05 - 0.18 m	Reddish yellow (5YR6/6-Dry); ; Sandy loam; Massive grade of structure; Dry; Weak 
	consistence; 0-2%, coarse fragments; Field pH 6.9 (pH meter); Abrupt change to - 
	B2	0.18 - 0.36 m	Strong brown (7.5YR5/8-Dry); ; Light clay; Moderate grade of structure, Angular blocky; Dry; 
	Firm consistence; 0-2%, coarse fragments; Very few (0 - 2 %), Gypseous, , Crystals; Field pH 
	6.9 (pH meter); Gradual change to - 
	B2	0.36 - 0.69 m	Strong brown (7.5YR5/8-Dry); ; Light clay; Moderate grade of structure, Angular blocky; Dry; 
	Firm consistence; Few (2 - 10 %), Gypseous, , Crystals; Field pH 6.2 (pH meter); Diffuse 
	B2	0.69 - 0.99 m	Strong brown (7.5YR5/8-Dry); ; Light clay; Moderate grade of structure, Angular blocky; Dry; 
	Firm consistence; Few (2 - 10 %), Gypseous, , Crystals; Field pH 6 (pH meter); Diffuse change 
	B2	0.99 - 1.3 m	Strong brown (7.5YR5/8-Dry); ; Light clay; Moderate grade of structure, Angular blocky; Dry; 
	Firm consistence; Few (2 - 10 %), Gypseous, , Crystals; Field pH 6 (pH meter); Diffuse change 
	B3	1.47 - 1.73 m	Pinkish yellow (7.5YR8/2-Dry); ; Light clay; Weak grade of structure, Angular blocky; Dry; Firm 
	consistence; Many (20 - 50 %), Gypseous, , Crystals; Field pH 6.5 (pH meter); Diffuse change 
	B3	1.73 - 2.03 m	Pink (7.5YR8/4-Dry); ; Light clay; Weak grade of structure, Angular blocky; Dry; Firm 
	consistence; Many (20 - 50 %), Gypseous, , Crystals; Field pH 6.1 (pH meter); 
	Morphological Notes
	Observation Notes
	COMPLETE SURFACE COVER OF GRAVEL FORMING HIGHLY POLISHED GRAVEL "PAVEMENT".                                             
	Site Notes
	DURRIE

	Project Name:	WQR
	Project Code:	WQR	Site ID:	B430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.7H	 0.4B
	0.05 - 0.18	6.9H	 2.68B
	0.18 - 0.36	6.9H	 2.72B
	0.36 - 0.69	6.2H	 8.11B
	0.69 - 0.99	6H	 9.8B
	0.99 - 1.3	6H	 11.5B
	1.47 - 1.73	6.5H	 29.8B
	1.73 - 2.03	6.1H	 28B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.14E	 26C	 0.017F	 0.02B	 7C	 72	 14	 8
	0.05 - 0.18
	0.18 - 0.36	 4C	 43	 8	 41
	0.36 - 0.69
	0.69 - 0.99
	0.99 - 1.3	 4C	 32	 8	 40
	1.47 - 1.73
	1.73 - 2.03
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.18
	0.18 - 0.36
	0.36 - 0.69
	0.69 - 0.99
	0.99 - 1.3
	1.47 - 1.73
	1.73 - 2.03

	Project Name:	WQR
	Project Code:	WQR	Site ID:	B430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded