Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	01/06/73	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.8	Runoff:	No Data
	Easting/Lat.:	-35.0666666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Brown Kandosol     	Principal Profile Form:	Uc4.11
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.06 m	Black (7.5YR2/0-Moist); ; Loamy sand; 
	A2	0.06 - 0.1 m	Brown (10YR5/3-Moist); ; Fine sandy loam; 20-50%, Shale, coarse fragments; Clear change to 
	0.1 - 0.2 m	; Silty loam; Massive grade of structure; Loose consistence; Diffuse change to - 
	0.2 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; 
	0.3 - 0.4 m	; Loam; 
	Morphological Notes
	Observation Notes
	WEATHERED SCHIST THROUGHOUT.  VERTICAL BEDDING WITH WEATHERED QUARTZITE AND MICA INTERLAYED.                  
	          
	Site Notes
	TOTNESS

	Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5A	 0.3C	 4.9K	 1.4	 0.83	 1
	0.06 - 0.1
	0.1 - 0.2	5.8A	 0.06C
	0.2 - 0.3
	0.3 - 0.4	5.4A	 0.06C	 1.3K	 0.3	 0.24	 0.58
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 9.8E	 14C	 61	 12	 5
	0.06 - 0.1
	0.1 - 0.2	 1.2E
	0.2 - 0.3
	0.3 - 0.4	 1E	 7C	 55	 16	 21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4

	Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1105	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction