Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1130	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:
	Date Desc.:	01/06/73	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.75	Runoff:	No Data
	Easting/Lat.:	-35	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn3.94
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Silty loam; 
	0.1 - 0.2 m	; Silty loam; 
	0.2 - 0.3 m	Pale brown (10YR6/3-Dry); ; 
	0.3 - 0.4 m	; Silty loam; 
	0.4 - 0.7 m	; 
	0.5 - 0.6 m	Brown (10YR5/3-Moist); ; 
	0.6 - 0.7 m	; 
	0.7 - 1 m	; 
	 -  m	; 
	0.9 - 1 m	Greyish brown (2.5Y5/2-Moist); , 7.5YR56; Silty loam; 
	Morphological Notes
	Observation Notes
	20-60CM FERROMANGANESE CONCRETIONS.                                                                                     
	Site Notes
	ALDGATE

	Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1130	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7A	 0.14C	 2.1K	 1.8	 1.6	 0.42
	0.1 - 0.2
	0.2 - 0.3	5.7A	 0.06C
	0.3 - 0.4	6.1A	 0.06C	 1.5K	 1.3	 0.28	 0.15
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7	7.2A	 0.06C
	0.7 - 0.8
	 - 
	0.9 - 1	6.9A	 0.06C	 1K	 3.4	 0.1	 0.35
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 5.9E	 19C	 33	 24	 14
	0.1 - 0.2
	0.2 - 0.3	 1.6E
	0.3 - 0.4	 1.3E	 17C	 35	 32	 16
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7	 0.4E
	0.7 - 0.8
	 - 
	0.9 - 1	 0.5E	 16C	 29	 28	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	 - 
	0.9 - 1

	Project Name:	Adelaide Hills Resource Study
	Project Code:	AHR	Site ID:	A1130	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction