Project Name:	Barossa District Zone IV, S.A.
	Project Code:	BA4	Site ID:	A171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:
	Date Desc.:	09/06/55	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	138.878333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-34.6594444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Magnesic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:
	Vegetation:
	Tall Strata - , , . *Species includes - Eucalyptus leucoxylon, Eucalyptus fastigata, Calotropis procera
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Greyish brown (2.5Y5/2-Moist); ; Sand; Single grain grade of structure; Diffuse change to - 
	0.1 - 0.3 m	Yellow (10YR7/6-Moist); ; Sand; Single grain grade of structure; Gradual change to - 
	0.3 - 0.38 m	Yellow (10YR7/6-Moist); ; Sand; Single grain grade of structure; Sharp change to - 
	0.38 - 0.46 m	Brownish yellow (10YR6/6-Moist); ; Sandy medium clay; Gradual change to - 
	0.46 - 0.61 m	Brownish yellow (10YR6/6-Moist); ; Medium clay; Gradual change to - 
	0.61 - 0.71 m	; Sandy medium clay; 
	1.22 - 1.37 m	; Sandy medium clay; 
	Morphological Notes
	Observation Notes
	Site Notes
	ADELAIDE

	Project Name:	Barossa District Zone IV, S.A.
	Project Code:	BA4	Site ID:	A171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.3H	 0.011C	 1.5K	 0.5	 0.19	 0.03	 3.1D
	 0.63
	0.1 - 0.3	6.4H	 0.01C
	0.3 - 0.38	6.6H	 0.01C
	0.38 - 0.46	6.5H	 0.013C	 0.4K	 3.8	 0.25	 0.2	 4.2D
	 3
	0.46 - 0.61	6.6H	 0.019C	 0.3K	 6	 0.21	 0.45	 5.6D
	 4.3
	0.61 - 0.71	5.7H	 0.032C
	1.22 - 1.37	4.7H	 0.09C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.004F	 0.053B	 34C	 59	 3	 4
	0.1 - 0.3
	0.3 - 0.38
	0.38 - 0.46	 0.006F	 0.041B
	0.46 - 0.61	 0.006F	 0.025B	 18C	 26	 3	 53
	0.61 - 0.71	 8C	 39	 1	 51
	1.22 - 1.37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.1 - 0.3
	0.3 - 0.38
	0.38 - 0.46
	0.46 - 0.61
	0.61 - 0.71
	1.22 - 1.37

	Project Name:	Barossa District Zone IV, S.A.
	Project Code:	BA4	Site ID:	A171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded