Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:	VOLUNTEER WEED PASTURE & SUB-CLOVER: 
	LARGELY WILD GERANIUM: 3/4 SHEEP PER ACRE
	Date Desc.:	04/10/54	Elevation:	No Data
	Map Ref.:	Sheet No. : 6728   1:100000	Rainfall:	0
	Northing/Long.:	139.123333333333	Runoff:	Rapid
	Easting/Lat.:	-34.7130555555556	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.02 m	Dark brown (7.5YR3/2-Moist); ; Coarse sand (Heavy); Single grain grade of structure; Very 
	weak consistence; FewGradual change to - 
	0.02 - 0.08 m	Dark brown (7.5YR3/2-Moist); ; Coarse sand (Heavy); Single grain grade of structure; Very 
	weak consistence; FewClear change to - 
	0.15 - 0.38 m	Strong brown (7.5YR5/5-Moist); ; Sand (Heavy); Single grain grade of structure; Weak 
	consistence; Clear change to - 
	0.46 - 0.76 m	Strong brown (7.5YR5/5-Moist); ; Sand (Heavy); Single grain grade of structure; Clear change 
	0.81 - 0.99 m	Yellowish red (5YR5/6-Moist); ; Sand (Heavy); Single grain grade of structure; Clear change to 
	0.99 - 1.07 m	Yellowish red (5YR4/7-Moist); ; Coarse sandy medium clay; Single grain grade of structure; 
	Strong consistence; Sharp, Irregular change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	STURT

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.5A	 0.026C
	0.02 - 0.08	 4.3	 0.4
	0.13 - 0.38	6.2A	 0.004C
	0.46 - 0.76	6.6A	 0.006C
	0.81 - 0.99	7A	 0.004C
	0.99 - 1.07	7.2A	 0.027C	 3F	 1.9	 19	 1.1	 1.6E
	 0.29	 0.31
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 0.163A
	0.02 - 0.08	 0.021F	 34C	 50	 8	 6
	0.13 - 0.38	 0.029A
	0.46 - 0.76
	0.81 - 0.99
	0.99 - 1.07	 0.013F	 19C	 44	 14	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.08
	0.13 - 0.38
	0.46 - 0.76
	0.81 - 0.99
	0.99 - 1.07

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A107	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded