Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	K.H. Northcote	Locality:	PASTURES: SUB-CLOVER
	Date Desc.:	06/10/54	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	139.090277777778	Runoff:	Rapid
	Easting/Lat.:	-34.6997222222222	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.04 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Heavy); Single grain grade of structure; Weak 
	consistence; Gradual change to - 
	A12	0.04 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Sand (Heavy); Weak grade of structure; Weak 
	consistence; Gradual change to - 
	A2	0.15 - 0.29 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Heavy); Very firm consistence; 2-10%, Schist, 
	coarse fragments; 
	Morphological Notes
	Observation Notes
	MICACEOUS THROUGHOUT                                                                                                    
	Site Notes
	STURT

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.5H	 0.021C	 6.5K	 1.5	 0.97	 0.15	 5.2D
	 11	 1.7
	0.04 - 0.15	6.5H	 0.013C
	0.15 - 0.29	6.3H	 0.009C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.03F	 0.216B	 17C	 63	 8	 10
	0.04 - 0.15
	0.15 - 0.29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.15
	0.15 - 0.29

	Project Name:	Barossa Valley V, S.A.
	Project Code:	BA5	Site ID:	A114	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded