Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	13/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 4966-1   1:50000	Rainfall:	No Data
	Northing/Long.:	8322479 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	668549  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Qa	Substrate Material:	Siltstone 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cryptogam surface, Hardsetting
	Erosion:	Active, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	33
	Mesotrophic Chomosolic Redoxic Hydrosol Thin Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clay-loamy Shallow
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida latifolia, Chrysopogon fallax, Heteropogon 
	contortus	Mid Strata - Shrub, 1.01-3m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Brown (10YR4/3-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-sticky; Field pH 6 
	(Raupach); Common, very fine (0-1mm) roots; Clear change to - 
	B2z	0.05 - 0.23 m	Yellowish brown (10YR5/4-Moist); , 7.5YR56, 10-20% , 5-15mm, Distinct; , 10YR51; Clay loam, 
	fine sandy; Massive grade of structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Slightly plastic; Very few (0 - 2 %), Ferromanganiferous, , Soft 
	segregations; Field pH 6 (Raupach); 
	2A1	0.23 - 0.32 m	Yellowish brown (10YR5/6-Moist); , 7.5YR56, 10-20% , 0-5mm, Distinct; , 10YR51; Fine sandy 
	loam; Massive grade of structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Few (2 - 10 %), Ferruginous, , Nodules; Field pH 6 (Raupach); 
	2B2	0.32 -  m	Yellowish brown (10YR5/4-Moist); , 10YR68, 10-20% ; , 10YR51; Light medium clay; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Dry; Common cutans, 10-50% of ped faces 
	or walls coated, distinct; Field pH 6 (Raupach); 
	Morphological Notes
	Observation Notes
	......
	Site Notes
	PHOTO NO; SURFACE - 6, E.PR...., M.SERICEA, TERMINCLIA PLATZPHYLLA, GYCOCARPA AMERILANA, TERMINELIA 
	CANESANS, ARISTIDA LATIFOLIA.  HYDROSOIL, ......., MESOTROPHIC THIN, NON-GRAVELLY, LOAMY, CL...., SHALLOW.

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile