Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	14/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 4966-1   1:50000	Rainfall:	No Data
	Northing/Long.:	8310089 AMG zone: 52	Runoff:	No runoff
	Easting/Lat.:	663819  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Backplain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Poached, Surface crust, Cryptogam surface
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	13
	Endohypersodic Massive Grey Vertosol Thick Fine Very fine  	Principal Profile Form:	N/A
	Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Sorghum timorense, Chrysopogon fallax, 
	Heteropogon contortus, Themeda triandra	Mid Strata - Shrub, 1.01-3m, Sparse. *Species includes - Carissa lanceolata
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Lysiphyllum cunninghamii, Eucalyptus papuana, Terminalia 
	platyphylla, Adansonia gregorii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR58, 10-20% , 0-5mm, Distinct; Light clay; Massive 
	grade of structure; Earthy fabric; Dry; Moderately plastic; Normal plasticity; Slightly sticky; Few 
	(2 - 10 %), Ferromanganiferous, , Nodules; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; 
	B21	0.05 - 0.4 m	Brown (7.5YR4/2-Moist); , 10YR41, 10-20% , 5-15mm, Distinct; , 10YR44; Heavy clay; 
	Moderate grade of structure, 10-20 mm, Subangular blocky; Rough-ped fabric; Moderately 
	moist; Very plastic; Normal plasticity; Very sticky; Few (2 - 10 %), Ferromanganiferous, , 
	Nodules; Field pH 7.5 (Raupach); Few, very fine (0-1mm) roots; 
	B22	0.4 - 0.8 m	Brown (7.5YR4/3-Moist); , 10YR78; Heavy clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Very plastic; Normal plasticity; Very sticky; Field pH 8.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	PHOTO NO; PROFILE - 12, LYSOPHLUM CUNNINGUMII, E.PRUNOSA, T.PLATYPHYLLA, E.PAPANA, CARISSA LANCEOLATE, 
	ADAMSONIA GREGORII, VERTOSOL, ......

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	206	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile