Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	17/10/96	Elevation:	No Data
	Map Ref.:	Sheet No. : 5067-3   1:50000	Rainfall:	No Data
	Northing/Long.:	8308362 AMG zone: 52	Runoff:	Very slow
	Easting/Lat.:	684040  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Paa	Substrate Material:	Soil pit, 0.2 m deep,Porous, Siltstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Pediment
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cryptogam surface, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	37
	Basic Lithic Leptic Rudosol Slightly gravelly Loamy   Very 	Principal Profile Form:	N/A
	shallow
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Aristida latifolia, Sorghum timorense
	Tall Strata - Tree, 1.01-3m, Mid-dense. *Species includes - Melaleuca minutifolia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; Moderate grade of structure, <2 mm; Rough-
	ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-plastic; Non-
	sticky; 0-2%, medium gravelly, 6-20mm, angular, Siltstone, coarse fragments; Field pH 6 
	(Raupach); Few, very fine (0-1mm) roots; Broken change to - 
	A2	0.03 - 0.1 m	Brown (10YR5/3-Moist); Light grey (2.5Y7/2-Moist); , 10YR58, 10-20% , 0-5mm, Distinct; Loam 
	(Heavy); Massive grade of structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Non-plastic; Non-sticky; 10-20%, medium gravelly, 6-20mm, angular, 
	coarse fragments; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; 
	BC	0.1 - 0.35 m	Light olive brown (2.5Y5/4-Moist); , 2.5Y66, 10-20% , 5-15mm, Faint; Loam; Massive grade of 
	structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Non-
	plastic; Non-sticky; 90-100%, medium gravelly, 6-20mm, subangular, coarse fragments; Field pH
	 6 (Raupach); Few, very fine (0-1mm) roots; 
	Cr	0.35 -  m	; Dry; 
	Morphological Notes
	Observation Notes
	Site Notes
	PHOTO NO; SURFACE - 1, REFER NOTES. M.MICROTHECC, SURG..., ANSTIDA, E.PU....

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.1

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile