Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A765	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	W.T. Ward	Locality:
	Date Desc.:	12/05/61	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	138.490277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-35.4527777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial fan
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Regolithic Calcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Alluvial soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Sod grass, <0.25m, . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	AC	0 - 0.05 m	Brown (7.5YR4/2-Moist); ; Silty loam; Weak grade of structure, Granular; Firm consistence; , 
	Calcareous, , Soft segregations; Many, very fine (0-1mm) roots; 
	C	0.08 - 0.13 m	Brown (7.5YR4/2-Moist); ; Silty loam; Single grain grade of structure; Firm consistence; , 
	Calcareous, , Soft segregations; Many, very fine (0-1mm) roots; 
	C	0.18 - 0.23 m	Brown (7.5YR4/2-Moist); ; Fine sandy loam; Single grain grade of structure; Firm consistence; , 
	Calcareous, , Soft segregations; Few, very fine (0-1mm) roots; 
	C	0.23 - 0.28 m	Brown (7.5YR4/4-Moist); ; Loamy fine sand; Single grain grade of structure; Very weak 
	consistence; , Calcareous, , Soft segregations; 
	AC	0.33 - 0.38 m	Dark greyish brown (10YR4/2-Moist); ; Silty loam; Single grain grade of structure; Firm 
	consistence; , Calcareous, , Soft segregations; 
	AC	0.41 - 0.46 m	Dark greyish brown (10YR4/2-Moist); ; Silty loam; Single grain grade of structure; Firm 
	consistence; , Calcareous, , Soft segregations; 
	AC	0.56 - 0.61 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Loose consistence; ,
	 Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	NOAR-WILL ADEL

	Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A765	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	8.5H	 0.077C	 5.8K	 2.4	 0.8	 2.5
	0.08 - 0.13	8.6H	 0.069C
	0.18 - 0.23	8.7H	 0.057C
	0.23 - 0.28	8.6H	 0.057C
	0.33 - 0.38	8.7H	 0.063C	 2.8K	 1.5	 0.3	 1.3
	0.41 - 0.46	8.7H	 0.057C
	0.56 - 0.61	8.9H	 0.042C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 9C	 3.1E	 0.033F	 0.27B	 0.85B	 1C	 16	 33	 36
	0.08 - 0.13	 10C	 2.2E	 0.2B	 1C	 21	 30	 35
	0.18 - 0.23	 7C	 0.13B	 1C	 45	 19	 27
	0.23 - 0.28	 5C	 0C	 54	 14	 21
	0.33 - 0.38	 10C	 0.022F	 0.13B	 0.78B	 2C	 11	 31	 39
	0.41 - 0.46	 9C	 2C	 24	 27	 35
	0.56 - 0.61	 17C	 4	 20C	 39	 8	 15
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.08 - 0.13
	0.18 - 0.23
	0.23 - 0.28
	0.33 - 0.38
	0.41 - 0.46
	0.56 - 0.61

	Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A765	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded