Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A777	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	W.T. Ward	Locality:
	Date Desc.:	13/10/61	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	138.469722222222	Runoff:	Moderately rapid
	Easting/Lat.:	-35.3377777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Grey Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Alluvial soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - , 0.26-0.5m, . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; Moderate grade of structure, Granular; Weak 
	consistence; AbundantDiffuse change to - 
	0.08 - 0.15 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; Weak grade of structure, Granular; Firm 
	consistence; AbundantDiffuse change to - 
	0.15 - 0.23 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; Massive grade of structure; Firm consistence; 
	FewDiffuse change to - 
	0.23 - 0.3 m	Dark grey (10YR4/1-Moist); ; Sandy clay loam; Massive grade of structure; Firm consistence; 
	FewDiffuse change to - 
	0.3 - 0.46 m	Dark grey (10YR4/1-Moist); ; Sandy clay loam; Massive grade of structure; Firm consistence; 
	FewDiffuse change to - 
	0.46 - 0.61 m	Grey (10YR5/1-Moist); ; Sandy clay loam; Massive grade of structure; Very firm consistence; 
	FewDiffuse change to - 
	0.61 - 0.76 m	Grey (10YR5/1-Moist); ; Silty loam; Massive grade of structure; Very firm consistence; Diffuse 
	change to - 
	0.76 - 0.86 m	Grey (7.5YR5/1-Moist); ; Silty loam (Heavy); Massive grade of structure; Firm consistence; 
	Diffuse change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	WILLUNGA ADEL

	Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A777	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.2H	 0.05C	 26K	 6.5	 1.4	 1
	0.08 - 0.15	7.1H	 0.024C
	0.15 - 0.23	7.1H	 0.021C
	0.23 - 0.3	7H	 0.024C
	0.3 - 0.46	7.3H	 0.019C	 14K	 8.2	 0.25	 1.1
	0.46 - 0.61	7.5H	 0.019C
	0.61 - 0.76	7.6H	 0.025C
	0.76 - 0.86	7.7H	 0.03C	 11K	 8.8	 0.25	 1.9
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 5.7E	 0.045F	 0.55B	 0.47B	 2	 4C	 43	 37	 16
	0.08 - 0.15	 0.26B	 1	 2C	 32	 39	 26
	0.15 - 0.23	 3.5E	 0.038F	 0.21B	 0.48B	 1C	 33	 39	 27
	0.23 - 0.3	 2C	 34	 35	 28
	0.3 - 0.46	 0.15B	 3C	 30	 34	 30
	0.46 - 0.61	 3C	 29	 34	 31
	0.61 - 0.76	 1.6E	 0.028F	 0.11B	 0.54B	 3C	 30	 29	 34
	0.76 - 0.86	 0.1B	 4C	 32	 27	 33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.23
	0.23 - 0.3
	0.3 - 0.46
	0.46 - 0.61
	0.61 - 0.76
	0.76 - 0.86

	Project Name:	Hd. Noarlunga & Willunga
	Project Code:	CA1	Site ID:	A777	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded