Project Name:	Cordillo, S.A.
	Project Code:	CO1	Site ID:	A563	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	22/07/58	Elevation:	No Data
	Map Ref.:	Sheet No. : SG54-14   1:250000	Rainfall:	0
	Northing/Long.:	140.65	Runoff:	No runoff
	Easting/Lat.:	-27.9166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	4 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Grey Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Pale brown (10YR6/3-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Columnar; 
	Firm consistence; 
	0.08 - 0.18 m	Pale brown (10YR6/3-Moist); ; Medium clay; 50-100 mm, Columnar; Coarse, (10 - 20) mm crack; 
	0.18 - 0.3 m	Pale brown (10YR6/3-Moist); ; Medium clay; Weak grade of structure, 50-100 mm, Columnar; 
	Massive grade of structure; 2-10%, Sand, coarse fragments; Very few (0 - 2 %), Calcareous, ,
	 Soft segregations; Clear change to - 
	0.3 - 0.48 m	Pale brown (10YR6/3-Moist); ; Medium clay; Massive grade of structure; Extremely coarse, (50 
	- 100) mm crack; Very firm consistence; 0-2%, Sand, coarse fragments; Very few (0 - 2 %), 
	Calcareous, , Soft segregations; Diffuse change to - 
	0.48 - 0.64 m	Pale brown (10YR6/3-Moist); ; Medium clay; Massive grade of structure; Strong consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.64 - 0.91 m	; Sandy medium clay; Very weak consistence; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.91 - 1.22 m	Reddish yellow (5YR6/7-Moist); ; Medium clay; Common (10 - 20 %), Calcareous, , Soft 
	segregations; Very few (0 - 2 %), Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes
	CORDILLO

	Project Name:	Cordillo, S.A.
	Project Code:	CO1	Site ID:	A563	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.5H	 0.024C
	0.08 - 0.18	8.9H	 0.038C
	0.18 - 0.3	9.3H	 0.065C
	0.3 - 0.48	9.7H	 0.098C
	0.48 - 0.64	9.8H	 0.16C
	0.64 - 0.91	9.6H	 0.28C
	0.91 - 1.22	8.6H	 0.8C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.03C	 0.027B	 13C	 42	 4	 37
	0.08 - 0.18	 0.06C
	0.18 - 0.3	 0.17C	 13C	 38	 3	 39
	0.3 - 0.48	 0.42C
	0.48 - 0.64	 0.69C	 13C	 38	 4	 41
	0.64 - 0.91	 1.3C
	0.91 - 1.22	 3.3C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.18
	0.18 - 0.3
	0.3 - 0.48
	0.48 - 0.64
	0.64 - 0.91
	0.91 - 1.22

	Project Name:	Cordillo, S.A.
	Project Code:	CO1	Site ID:	A563	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded