Project Name:	Elizabeth, S.A.
	Project Code:	EA1	Site ID:	A534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.B. Wells	Locality:
	Date Desc.:	21/04/58	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	Moderately rapid
	Easting/Lat.:	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	No Data
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Red Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR5/4-Moist); ; Fine sandy loam; Massive grade of structure; Strong consistence; 
	Diffuse change to - 
	A2B	0.1 - 0.18 m	Reddish brown (5YR5/4-Moist); ; Fine sandy loam (Heavy); Massive grade of structure; Strong 
	consistence; Sharp change to - 
	B1	0.18 - 0.38 m	Dark reddish brown (5YR3/2-Moist); ; Medium clay; 10-20 mm, Angular blocky; 5-10 mm, 
	Angular blocky; Very firm consistence; Gradual change to - 
	B2	0.38 - 0.58 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; 10-20 mm, Angular blocky; , Granular; Firm 
	consistence; Gradual change to - 
	B1k	0.58 - 0.81 m	Reddish brown (5YR4/4-Moist); ; Medium clay; 10-20 mm, Angular blocky; , Granular; Very 
	weak consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	B2k	0.86 - 0.96 m	Reddish brown (5YR5/4-Moist); ; Fine sandy loam; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Clear change to - 
	0.96 - 1.09 m	Reddish brown (5YR4/4-Moist); ; Loam; Sharp change to - 
	1.09 - 1.27 m	Dark red (2.5YR3/6-Moist); ; Clay loam; 20-50 mm, Angular blocky; , Granular; Very weak 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Clear change to - 
	1.27 - 1.47 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Weak grade of structure, 20-50 mm, Angular blocky; 
	Weak grade of structure, Granular; Very weak consistence; Common (10 - 20 %), Calcareous, 
	, Soft segregations; Gradual change to - 
	1.47 - 1.75 m	Yellowish red (5YR4/6-Moist); ; Clay loam; Weak grade of structure, 20-50 mm, Angular blocky; 
	Weak grade of structure, Granular; Very weak consistence; Few (2 - 10 %), Calcareous, , Soft
	 segregations; 
	1.93 - 2.13 m	Reddish brown (5YR4/3-Moist); ; Loam; Strong grade of structure, 20-50 mm, Angular blocky; , 
	Granular; Very weak consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; Clear 
	change to - 
	3A	2.13 - 2.23 m	Yellowish red (5YR4/6-Moist); ; Clay loam, fine sandy (Heavy); Weak grade of structure, 
	Granular; ; FragmentVery weak consistence; Clear change to - 

	Project Name:	Elizabeth, S.A.
	Project Code:	EA1	Site ID:	A534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	2.23 - 2.46 m	Dark reddish brown (2.5YR3/4-Moist); ; Clay loam; 50-100 mm, Prismatic; , Granular; Very weak
	 consistence; Few (2 - 10 %), Calcareous, , Nodules; Gradual change to - 
	2.46 - 2.59 m	Dark reddish brown (2.5YR3/4-Moist); ; Clay loam; 50-100 mm, Prismatic; , Granular; Very weak
	 consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	2.69 - 2.97 m	Dark red (2.5YR3/6-Moist); ; Clay loam; 50-100 mm, Prismatic; , Granular; Very weak 
	consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Clear change to - 
	2.97 - 3.22 m	Dark reddish brown (2.5YR3/4-Moist); ; Clay loam; 20-50 mm, Prismatic; , Granular; Very weak 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Sharp change to - 
	3.22 - 3.35 m	Red (2.5YR4/6-Moist); ; Medium clay; , Angular blocky; , Granular; Very weak consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	ALL GLAZED PEDS:                                                                                                        
	Site Notes
	ADELAIDE

	Project Name:	Elizabeth, S.A.
	Project Code:	EA1	Site ID:	A534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.1H	 0.02C	 5.1K	 2	 0.69	 0.59
	0.1 - 0.18	7.5H	 0.04C	 4.7K	 3.1	 0.27	 1.7
	0.18 - 0.38	8.6H	 0.12C	 10.5K	 14	 0.78	 7
	0.38 - 0.58	9.8H	 0.29C	 8.9K	 18	 1.08	 10.1
	0.58 - 0.81	10H	 0.42C
	0.86 - 0.96	9.8H	 0.36C
	0.96 - 1.09	9.8H	 0.45C
	1.09 - 1.27	10.1H	 0.72C	 7K	 15	 1.4	 11
	1.27 - 1.47	9.9H	 0.67C
	1.47 - 1.75	10H	 0.58C
	1.93 - 2.13	10H	 0.5C
	2.13 - 2.23	9.8H	 0.33C
	2.23 - 2.46	10.1H	 0.59C	 5.2K	 14	 1.6	 10
	2.46 - 2.59	10.2H	 0.57C
	2.69 - 2.97	10H	 0.47C
	2.97 - 3.22	10.1H	 0.45C	 4.4K	 11	 1.2	 8
	3.22 - 3.35	10H	 0.39C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.022F	 0.082B	 0.38B	 6C	 56	 23	 15
	0.1 - 0.18	 0.057B	 6C	 53	 24	 16
	0.18 - 0.38	 0.01C	 0.086B	 3C	 32	 17	 48
	0.38 - 0.58	 0.03C	 0.021F	 0.056B	 0.81B	 2C	 29	 16	 50
	0.58 - 0.81	 11C	 8C	 29	 14	 35
	0.86 - 0.96	 5.7C	 5C	 46	 24	 22
	0.96 - 1.09	 1.7C	 3C	 42	 25	 28
	1.09 - 1.27	 13C	 1C	 15	 11	 61
	1.27 - 1.47	 23C	 1C	 19	 11	 44
	1.47 - 1.75	 17C	 1C	 23	 17	 39
	1.93 - 2.13	 0.44C	 3C	 30	 20	 44
	2.13 - 2.23	 0.93C	 7C	 51	 18	 21
	2.23 - 2.46	 1.6C	 5C	 23	 7	 65
	2.46 - 2.59	 10C	 6C	 22	 2	 58
	2.69 - 2.97	 22C	 4C	 21	 5	 44
	2.97 - 3.22	 12C	 5C	 29	 8	 43
	3.22 - 3.35	 19C	 5C	 33	 9	 33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.18
	0.18 - 0.38
	0.38 - 0.58
	0.58 - 0.81
	0.86 - 0.96
	0.96 - 1.09

	Project Name:	Elizabeth, S.A.
	Project Code:	EA1	Site ID:	A534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	1.09 - 1.27
	1.27 - 1.47
	1.47 - 1.75
	1.93 - 2.13
	2.13 - 2.23
	2.23 - 2.46
	2.46 - 2.59
	2.69 - 2.97
	2.97 - 3.22
	3.22 - 3.35

	Project Name:	Elizabeth, S.A.
	Project Code:	EA1	Site ID:	A534	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded