Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1212	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:	South-west of Lake Yaninee, Pordia district.
	Date Desc.:	19/04/83	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	135.16666667	Runoff:	Rapid
	Easting/Lat.:	-33.01666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc1.34
	ASC Confidence:	Great Soil Group:	Calcareous sand
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Black (5YR2.5/1-Moist); ; Loamy sand; Massive grade of structure; Very weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Very few (0 - 2 %), Calcareous, , 
	0.1 - 0.2 m	Very dark grey (5YR3/1-Moist); ; Sandy loam (Light); Massive grade of structure; Very weak 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Few (2 - 10 %), 
	Calcareous, , Concretions; Diffuse change to - 
	0.2 - 0.3 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Massive grade of structure; Very weak 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Very many (50 - 100 %), 
	Calcareous, , Concretions; Sharp change to - 
	Morphological Notes
	Calcrete underlies the third sample.
	Observation Notes
	Vegetation:Open malle eucalypt woodland.  Parent material: Aeolian.  Field PPF = Uc5.12.
	Site Notes
	Landform: stripped dune crest.

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1212	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.5A	1.8A	15K	5.4	1.3	2.6	21J	25D	12.38
	0.1 - 0.2	8.8A	2.27A	11K	6.5	1.6	3.9	18J	23D	21.67
	0.2 - 0.3	9.1A	>3A	4.4K	6.4	1.8	5.5	12J	18D	45.83
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	6.5B	2.93A	23E	0.19A	30D	39	3	14
	0.1 - 0.2	7.8B	2.76A	29D	39	3	14
	0.2 - 0.3	17B	1.57A	26D	36	1	14
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1212	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_BASES	Sum of Bases
	18B2	Sulfuric acid (10%)- extractable potassium
	19B1	Carbonates - manometric
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10_PB1_C	Clay (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_CS	Coarse sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_FS	Fine sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_Z	Silt (%) - Plummet balance (Acid digestion pretreatment)