Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1225	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:	South of Colley on the road to Port Kenny, Venus 
	district.
	Date Desc.:	20/10/83	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	134.7	Runoff:	Rapid
	Easting/Lat.:	-33.08333333	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gc1.12
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); ; Fine sandy loam; Massive grade of 
	structure; Very weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Few 
	(2 - 10 %), Calcareous, Fine (0 - 2 mm), Concretions; Abundant, coarse (>5mm) roots; 
	0.1 - 0.2 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); ; Fine sandy loam; Massive grade of 
	structure; Very weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Few 
	(2 - 10 %), Calcareous, Fine (0 - 2 mm), Concretions; Abundant, coarse (>5mm) roots; 
	0.2 - 0.3 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Fine sandy loam; Massive grade of 
	structure; Very weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Few 
	(2 - 10 %), Calcareous, Fine (0 - 2 mm), Concretions; Few
	0.3 - 0.4 m	Yellowish brown (10YR5/4-Moist); Light yellowish brown (10YR6/4-Dry); ; Fine sandy loam; 
	Massive grade of structure; Very weak consistence; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Many (20 - 50 %), Calcareous, , Concretions; Few
	0.4 - 0.6 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Sandy loam; Massive grade of structure; Very 
	weak consistence; 2-10%, coarse fragments; Many (20 - 50 %), Calcareous, , Soft 
	segregations; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Concretions; 
	0.6 - 0.8 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Fine sandy loam; Massive grade of structure; 
	Weak consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Common (10 - 20 %), 
	Calcareous, , Concretions; 
	0.8 - 1 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Fine sandy clay loam (Light); Massive grade of 
	structure; Weak consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Many (20 - 50
	 %), Calcareous, , Nodules; 
	1 - 1.2 m	Brown (7.5YR5/4-Moist); Pink (7.5YR7/4-Dry); ; Fine sandy clay loam; Massive grade of 
	structure; Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Very 
	many (50 - 100 %), Calcareous, , Nodules; 
	1.2 - 1.4 m	Reddish yellow (7.5YR6/5-Moist); Pink (7.5YR7/4-Dry); ; Clay loam; Massive grade of structure; 
	Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Very many (50 - 
	100 %), Calcareous, , Nodules; 
	Morphological Notes

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1225	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Some rounded fragments of pupal cases.
	Gravels - feranginous and quartzitic.
	Derived from granite.
	Observation Notes
	Vegetation: dense low mallee/broombush woodland.  Soil family: Unit 40 (Colley).
	Site Notes
	Landform: Mid-slope to granite high.

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1225	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.5A	0.98A	20K	8.2	2.1	2	34J	32D	5.88
	0.1 - 0.2	8.7A	1.77A
	0.2 - 0.3	9.2A	2.28A	7.6K	6.7	2.5	8.4	23J	25D	36.52
	0.3 - 0.4	9.7A	2.38A
	0.4 - 0.6	9.8A	2.42A	1.5K	5.4	2.2	10	15J	19D	66.67
	0.6 - 0.8	9.7A	2.44A
	0.8 - 1	9.5A	2.31A
	1 - 1.2	9.6A	2.55A	2.1K	5.3	1.7	9.2	20J	18D	46.00
	1.2 - 1.4	9.6A	2.54A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	23B	4.48A	24E	0.21A	13D	25	12	20
	0.1 - 0.2	27B	2.94A	11D	24	10	19
	0.2 - 0.3	26B	2.25A	10D	23	10	25
	0.3 - 0.4	37B	0.89A	9D	22	8	17
	0.4 - 0.6	41B	0.82A	11D	20	9	15
	0.6 - 0.8	41B	0.84A	11D	19	10	13
	0.8 - 1	49B	0.43A	8D	18	8	14
	1 - 1.2	50B	0.72A	7D	16	8	17
	1.2 - 1.4	58B	0.15A	4D	12	8	16
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2
	1.2 - 1.4

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1225	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_BASES	Sum of Bases
	18B2	Sulfuric acid (10%)- extractable potassium
	19B1	Carbonates - manometric
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10_PB1_C	Clay (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_CS	Coarse sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_FS	Fine sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_Z	Silt (%) - Plummet balance (Acid digestion pretreatment)