Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	Malcolm J. Wright	Locality:	Near Piednippie Hall on Highway, Courela district.
	Date Desc.:	21/10/83	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	134.41666667	Runoff:	Rapid
	Easting/Lat.:	-32.73333333	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc1.13
	ASC Confidence:	Great Soil Group:	Calcareous sand
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Brown (7.5YR4/3-Moist); Brown (7.5YR5/3-Dry); ; Loamy sand; Massive grade of structure; 
	Weak consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Very few (0 - 2 %), 
	Calcareous, Fine (0 - 2 mm), Concretions; Abundant, fine (1-2mm) roots; 
	0.1 - 0.2 m	Brown (7.5YR4/3-Moist); Brown (7.5YR5/3-Dry); ; Loamy sand; Massive grade of structure; 
	Weak consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Few (2 - 10 %), 
	Calcareous, Fine (0 - 2 mm), Concretions; Few, fine (1-2mm) roots; 
	0.2 - 0.3 m	Brown (7.5YR4/3-Moist); Brown (7.5YR5/3-Dry); ; Loamy sand; Massive grade of structure; 
	Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Few (2 - 10 %), 
	Calcareous, Fine (0 - 2 mm), Concretions; Few, fine (1-2mm) roots; 
	0.3 - 0.5 m	Brown (7.5YR4/4-Moist); Pale brown (10YR6/3-Dry); ; Loamy sand; Massive grade of 
	structure; Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; Few, 
	fine (1-2mm) roots; 
	0.5 - 0.7 m	Brown (7.5YR5/4-Moist); Very pale brown (10YR7/3-Dry); ; Loamy sand; Massive grade of 
	structure; Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; 
	Common (10 - 20 %), Calcareous, , Nodules; 
	0.7 - 0.9 m	Brown (7.5YR5/4-Moist); Very pale brown (10YR7/3-Dry); ; Loamy sand; Massive grade of 
	structure; Weak consistence; Very many (50 - 100 %), Calcareous, , Soft segregations; 
	Common (10 - 20 %), Calcareous, , Nodules; 
	Morphological Notes
	Calcrete cap (Bakhava).
	Observation Notes
	Vegetation is cleared.  Soil Family: Unit 20 (Bald Hills).  Parent material = Aeolian.  Field PPF = Uc5.12?
	Site Notes
	Landform: near crest of moderately high rise.

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.5A	0.15A	9.1K	1.2	0.85	0.28	11D
	0.1 - 0.2	8.7A	0.13A
	0.2 - 0.3	8.7A	0.13A	7.8K	1.3	0.57	0.27	10J	10D	2.70
	0.3 - 0.5	8.8A	0.13A
	0.5 - 0.7	9.1A	0.13A
	0.7 - 0.9	9.3A	0.16A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	68B	1.99A	14E	0.15A	2D	11	6	9
	0.1 - 0.2	71B	1.44A	1D	11	6	8
	0.2 - 0.3	71B	1.53A	1D	11	5	8
	0.3 - 0.5	78B	0.79A
	0.5 - 0.7	79B	0.77A
	0.7 - 0.9	78B	0.8A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.7
	0.7 - 0.9

	Project Name:	Eyre Peninsula Soil Survey
	Project Code:	EP	Site ID:	A1229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_BASES	Sum of Bases
	18B2	Sulfuric acid (10%)- extractable potassium
	19B1	Carbonates - manometric
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B2	Bicarbonate-extractable phosphorus - automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10_PB1_C	Clay (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_CS	Coarse sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_FS	Fine sand (%) - Plummet balance (Acid digestion pretreatment)
	P10_PB1_Z	Silt (%) - Plummet balance (Acid digestion pretreatment)