Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	16/04/56	Elevation:	 64 metres
	Map Ref.:	Rainfall:	690
	Northing/Long.:	140.82	Runoff:	Rapid
	Easting/Lat.:	-37.7716666666667	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Ridge	Relief:	9 metres
	Elem. Type:	Dune	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Very dark brown (10YR2/2-Moist); Dark greyish brown (10YR4/2-Dry); ; Sandy loam (Light); , 
	Granular; Weak consistence; Abundant
	0.08 - 0.15 m	Very dark brown (10YR2/2-Moist); ; Loamy sand; Weak grade of structure, Granular; Weak 
	consistence; ManyDiffuse change to - 
	0.15 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Sand (Heavy); Firm consistence; Diffuse change to - 
	0.3 - 0.45 m	Dark yellowish brown (10YR3/4-Moist); Yellowish brown (10YR5/5-Dry); ; Sand; Firm 
	consistence; Diffuse change to - 
	0.45 - 0.55 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Very weak consistence; Diffuse change to - 
	0.55 - 1.01 m	Yellowish brown (10YR5/4-Moist); Brownish yellow (10YR6/6-Dry); ; Sand; Loose 
	consistence; 0-2%, Other, coarse fragments; Diffuse change to - 
	Morphological Notes
	Observation Notes
	PROFILE SHOWS DEPOSIT OF VOLCANIC ASH ON PODZOL: LAYER 4 - CHARCOAL FRAGMENTS:                                          
	Site Notes
	GREY

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.8H	 0.038C	 11K	 1.6	 0.17	 0.58
	0.08 - 0.15	6.6H	 0.019C
	0.15 - 0.3	6.6H	 0.021C	 5.1K	 1	 0.07	 0.15
	0.3 - 0.45
	0.45 - 0.55	6.5H	 0.044C
	0.55 - 1.01	6.8H	 0.003C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.046F	 0.33B	 0.02B	 26C	 62	 7	 5
	0.08 - 0.15	 0.038F	 0.26B	 25C	 63	 7	 5
	0.15 - 0.3	 15C	 0.031F	 0.13B	 0.01B	 25C	 66	 6	 3
	0.3 - 0.45	 0.037F	 28C	 64	 5	 3
	0.45 - 0.55	 33C	 63	 4	 0
	0.55 - 1.01	 0.006F	 0.01B	 0.01B	 16C	 81	 1	 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.3
	0.3 - 0.45
	0.45 - 0.55
	0.55 - 1.01

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	12_NR_ZN	Total element - Zn(mg/kg) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded