Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	19/04/56	Elevation:	 61 metres
	Map Ref.:	Rainfall:	610
	Northing/Long.:	140.772777777778	Runoff:	Moderately rapid
	Easting/Lat.:	-37.3288888888889	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Plain
	Morph. Type:	Ridge	Relief:	6 metres
	Elem. Type:	Lunette	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Black earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Black (10YR2/1-Moist); ; Medium clay; , Granular; Weak consistence; Diffuse change to - 
	0.1 - 0.3 m	Black (10YR2/1-Moist); ; Medium clay; , Granular; Weak consistence; 
	0.33 - 0.38 m	Very dark grey (10YR3/1-Moist); , 10YR61; Medium clay; Weak consistence; 
	0.4 - 0.48 m	Grey (10YR6/1-Moist); , 10YR63; Firm consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	GREY

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.3H	 0.068C	 51K	 5.8	 5.2	 0.42	 73J	0.58
	0.1 - 0.3	7.7H	 0.041C
	0.33 - 0.38	8.4H	 0.059C	 52J
	0.4 - 0.48
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.046F	 0.54B	 1.4B	 5C	 21	 17	 54
	0.1 - 0.3
	0.33 - 0.38	 18C	 0.038F	 0.12B	 1.25B	 3C	 15	 7	 55
	0.4 - 0.48
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.33 - 0.38
	0.4 - 0.48

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A310	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction