Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A355	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	10/05/56	Elevation:	 40 metres
	Map Ref.:	Rainfall:	670
	Northing/Long.:	140.820277777778	Runoff:	Very rapid
	Easting/Lat.:	-37.8377777777778	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Plain
	10%
	Morph. Type:	Simple-slope	Relief:	30 metres
	Elem. Type:	Beach ridge	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Regolithic Chernic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Very dark grey (10YR3/1-Moist); Very dark greyish brown (10YR3/2-Dry); ; Loamy sand; , 
	Granular; Weak consistence; 
	0.08 - 0.23 m	Very dark grey (10YR3/1-Moist); ; Loamy sand; , Granular; Weak consistence; Diffuse change 
	to - 
	0.23 - 0.53 m	Very dark greyish brown (10YR3/2-Moist); Dark greyish brown (10YR4/2-Dry); ; Loamy sand; ,
	 Granular; Firm consistence; 
	0.53 - 0.73 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Sharp change to - 
	0.73 - 0.76 m	Yellowish brown (10YR5/5-Moist); , 10YR44; Loamy sand; 2-10%, Tuff, coarse fragments; 
	1.42 - 1.7 m	White (10YR8/1-Dry); ; Sand; 
	Morphological Notes
	Observation Notes
	Site Notes
	GREY

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A355	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	7.3H	 0.023C	 9.2K	 2.2	 0.48	 0.4
	0.08 - 0.23	7.3H	 0.028C
	0.23 - 0.53	7.7H	 0.005C
	0.53 - 0.73	7.8H	 0.022C
	0.73 - 0.76	8H	 0.016C
	1.42 - 1.7	7.2H	 0.004C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.046F	 0.44B	 0.04B	 13C	 75	 9	 3
	0.08 - 0.23	 0.31B	 11C	 75	 11	 3
	0.23 - 0.53	 0.17B
	0.53 - 0.73	 0.04C	 16C	 72	 10	 2
	0.73 - 0.76	 0.04C	 0.84B
	1.42 - 1.7	 3C	 94	 2	 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.23
	0.23 - 0.53
	0.53 - 0.73
	0.73 - 0.76
	1.42 - 1.7

	Project Name:	Co. Grey Rec., S.A.
	Project Code:	GR1	Site ID:	A355	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded