Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A985	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:
	Date Desc.:	01/10/66	Elevation:	 6 metres
	Map Ref.:	Sheet No. : SI53-4   1:250000	Rainfall:	0
	Northing/Long.:	137.575277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-32.9369444444445	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.16 m	Red (2.5YR5/6-Dry); ; Sandy clay loam; Massive grade of structure; Very weak consistence; 
	Diffuse change to - 
	0.16 - 0.33 m	Red (2.5YR4/6-Dry); ; Sandy clay loam; Massive grade of structure; Very weak consistence; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.33 - 0.62 m	Red (2.5YR5/6-Dry); ; Massive grade of structure; Firm consistence; Many (20 - 50 %), 
	Calcareous, , Soft segregations; Diffuse change to - 
	0.62 - 0.93 m	Red (2.5YR5/6-Dry); ; Sandy clay loam; Massive grade of structure; Very weak consistence; 
	Many (20 - 50 %), Calcareous, , Soft segregations; 
	0.93 - 1.23 m	; 
	 -  m	; 
	 -  m	; 
	 -  m	; 
	 -  m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	WHYALLA 3

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A985	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.1J	 0.073A	 6.3B	 3	 1.3	 0.49	 33J	1.48
	8.2A
	0.1 - 0.2	7.2J	 0.141A	 8.6B	 3.7	 1.3	 1.3	 33J	3.94
	8.9A
	0.2 - 0.3	7.5J	 0.324A	 16B	 5.9	 1.3	 2.7
	9.1A
	0.3 - 0.4	7.7J	 0.703A	 25B	 8.9	 1	 5.2
	9.2A
	0.4 - 0.5	7.8J	 1.19A
	9.2A
	0.5 - 0.6	7.8J	 1.51A	 23B	 7.1	 0.78	 4.5
	9.2A
	0.6 - 0.7	7.8J	 1.27A
	9.3A
	0.7 - 0.8	7.8J	 1.22A
	9.4A
	0.8 - 0.9	7.8J	 1.27A
	9.4A
	0.93 - 1.23
	 - 
	 - 
	 - 
	 - 
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.07C	 0.523A	 9A	 0.02A	 0.046B	 1.2A	1.60	 6	 38C	 39	 10	 13
	0.1 - 0.2	 0.1C	 0.291A	 6A	 0.02A	 0.04B	 1.2A	1.30	 7	 35C	 34	 6	 21
	0.2 - 0.3	 0.5C	 0.02A	 0.047B	 1.3A	1.50	 7	 29C	 32	 7	 28
	0.3 - 0.4	 7.6C	 0.291A	 5A	 0.02A	 0.046B	 1.3A	1.50	 8	 27C	 23	 5	 32
	0.4 - 0.5	 15C
	0.5 - 0.6	 25C	 0.174A	 4A	 0.03A	 0.022B	 0.95A	1.50	 9	 22C	 19	 7	 23
	0.6 - 0.7
	0.7 - 0.8	 22C	 0.116A	 3A	 0.02A	 0.012B	 0.96A	 10	 26C	 21	 4	 26
	0.8 - 0.9
	0.93 - 1.23
	 - 
	 - 
	 - 
	 - 
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.2C	 0.07C
	0.1 - 0.2	 0.2C	 0.09C
	0.2 - 0.3	 0.26C	 0.13C
	0.3 - 0.4	 0.3C	 0.13C
	0.4 - 0.5

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A985	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	0.5 - 0.6	 0.3A	 0.13A
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.93 - 1.23
	 - 
	 - 
	 - 
	 - 

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A985	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_C_2.5	pH of soil - pH of 1:2.5 Soil/0.1M CaCl2 suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	MIN_NR_K2O	Kaolin minerals
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_NR_01	0.1 BAR Moisture % - Not recorded
	P3B_NR_15	15 BAR Moisture % - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction