Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A992	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	R.W. Jessup	Locality:	COALESCING ALLUVIAL FANS FORMING GENTLY-
	SLOPING COASTAL PLAIN
	Date Desc.:	01/11/66	Elevation:	 5 metres
	Map Ref.:	Sheet No. : SI53-4   1:250000	Rainfall:	254
	Northing/Long.:	137.759444444444	Runoff:	Moderately rapid
	Easting/Lat.:	-32.5652777777778	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial fan
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Pedaric Red Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Desert loam
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - Atriplex vesicaria
	Surface Coarse Fragments:	90-100%, , , Gravel
	Profile Morphology
	A	0 - 0.03 m	Yellowish red (5YR4/6-Moist); ; Loam; Massive grade of structure; 0-2%, coarse fragments; 
	Sharp change to - 
	B	0.03 - 0.08 m	Red (2.5YR4/6-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Diffuse change to - 
	Bk	0.08 - 0.15 m	Red (2.5YR4/6-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change to - 
	Bk	0.15 - 0.25 m	Red (2.5YR5/8-Moist); ; Light clay; Massive grade of structure; Very weak consistence; Many 
	(20 - 50 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.25 - 0.37 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Very firm consistence; 0-2%, 
	coarse gravelly, 20-60mm, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Very few (0 - 2 %), Gypseous, , Soft segregations; Sharp change to - 
	0.37 - 0.58 m	Yellowish red (5YR4/6-Moist); ; Light clay; Massive grade of structure; Very firm consistence; 
	10-20%, coarse gravelly, 20-60mm, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Many (20 - 50 %), Gypseous, , Soft segregations; Clear change to - 
	0.58 - 0.68 m	; Light clay; 20-50%, medium gravelly, 6-20mm, Gravel, coarse fragments; Many (20 - 50 %), 
	Calcareous, , Soft segregations; 
	0.68 - 0.98 m	; 
	Morphological Notes
	light clay with shell fragments & black gravel
	Observation Notes
	Site Notes
	PT. AUGUSTA

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A992	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	7.7J	 0.432A	 12K	 4.2	 2	 1.1
	8.3H
	0.03 - 0.08	7.8J	 7.84A	 41J
	7.7H
	0.08 - 0.15	8J	 11.9A	 40J
	7.9H
	0.15 - 0.25	8.2J	 13A
	8H
	0.25 - 0.37	8.1J	 14.9A
	8H
	0.37 - 0.47	8.1J	 35.1A
	8H
	0.47 - 0.58	8.2J	 24.1A
	8.1H
	0.58 - 0.68	8.2J	 9.46A
	8H
	0.68 - 0.98
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.54C	 0.814A	 21A	 0.03A	 0.092B	 1.3A	1.30	 32	 17C	 59	 4	 16
	0.03 - 0.08	 1.4C	 1.16A	 16A	 0.04A	 0.12B	 2A	1.30	 1	 13C	 28	 29	 22
	0.08 - 0.15	 16C	 1.05A	 22A	 0.04A	 0.095B	 1.8A	1.30	 1	 10C	 27	 25	 18
	0.15 - 0.25	 16C	 0.03A	 1.4A	1.10	 3	 8C	 26	 19	 21
	0.25 - 0.37	 1.5C	 0.174A	 18A	 0.02A	 0.028B	 1.6A	 5	 7C	 31	 17	 36
	0.37 - 0.47	 4.3C	 0.03A	 1.4A
	0.47 - 0.58	 6.3C	 51	 10C	 31	 17	 24
	0.58 - 0.68	 18C	 0.174A	 17A	 0.04A	 0.014B	 1.2A	 51	 12C	 32	 3	 30
	0.68 - 0.98
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03	 0.27C	 0.16C
	0.03 - 0.08	 0.27C	 0.16C
	0.08 - 0.15	 0.45C	 0.27C
	0.15 - 0.25	 0.44A	 0.23A
	0.25 - 0.37
	0.37 - 0.47
	0.47 - 0.58
	0.58 - 0.68
	0.68 - 0.98

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS1	Site ID:	A992	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A1	Total potassium - X-ray fluorescence
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4_NR	pH of soil - Not recorded
	4B_C_2.5	pH of soil - pH of 1:2.5 Soil/0.1M CaCl2 suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	MIN_NR_K2O	Kaolin minerals
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_NR_01	0.1 BAR Moisture % - Not recorded
	P3B_NR_15	15 BAR Moisture % - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction