Project Name:	1968 ISSS Congress Tour
	Project Code:	IS5	Site ID:	A980	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G. Blackburn	Locality:
	Date Desc.:	28/09/66	Elevation:	 50 metres
	Map Ref.:	Sheet No. : SJ54-2   1:250000	Rainfall:	0
	Northing/Long.:	140.91666667	Runoff:	Moderately rapid
	Easting/Lat.:	-36.88333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Beach ridge plain
	Morph. Type:	Ridge	Relief:	10 metres
	Elem. Type:	Beach ridge	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Fragic Sesquic Aeric Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sedge, , . *Species includes - None recorded
	Mid Strata - , , . *Species includes - Bassia species
	Tall Strata - Tree, 20.01-35m, . *Species includes - Eucalyptus baxteri
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.03 m	Greyish brown (2.5Y5/2-Moist); ; , Granular; Weak consistence; Diffuse change to - 
	A1	0.03 - 0.1 m	Grey (10YR5/1-Moist); ; , Granular; Weak consistence; Diffuse change to - 
	A1	0.1 - 0.2 m	White (10YR8/1-Moist); ; , Granular; Weak consistence; Diffuse change to - 
	A1	0.2 - 0.3 m	Light grey (10YR7/1-Moist); ; , Granular; Weak consistence; Diffuse change to - 
	A12	0.3 - 0.4 m	Grey (10YR6/1-Moist); ; Single grain grade of structure; Weak consistence; Diffuse change to - 
	A2	0.4 - 0.5 m	White (10YR8/2-Moist); ; Single grain grade of structure; Weak consistence; Diffuse change to - 
	A2	0.5 - 0.6 m	Light grey (10YR7/2-Moist); ; Single grain grade of structure; Weak consistence; Diffuse 
	change to - 
	A2	0.6 - 0.8 m	Light grey (10YR7/2-Moist); ; Single grain grade of structure; Weak consistence; Diffuse 
	change to - 
	A2B	0.8 - 0.9 m	Very pale brown (10YR8/3-Moist); ; Single grain grade of structure; Weak consistence; Diffuse 
	change to - 
	B1	0.9 - 1 m	Yellow (10YR8/5-Moist); ; Single grain grade of structure; Weak consistence; Diffuse change to
	B1	1 - 1.16 m	Yellow (10YR7/6-Moist); ; Single grain grade of structure; Weak consistence; Diffuse change to
	B1	1.16 - 1.36 m	Yellowish brown (10YR5/4-Moist); , 10YR78; , 10YR43; Single grain grade of structure; Very 
	firm consistence; Diffuse change to - 
	B1	1.36 - 1.6 m	Brownish yellow (10YR6/8-Moist); , 10YR43; , 10YR56; Single grain grade of structure; Firm 
	consistence; Diffuse change to - 
	1.6 - 1.75 m	Dark yellowish brown (10YR4/4-Moist); , 10YR76; , 10YR88; Single grain grade of structure; 
	Firm consistence; 

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS5	Site ID:	A980	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	1.75 - 1.9 m	Dark yellowish brown (10YR4/4-Moist); , 10YR76; , 10YR88; Single grain grade of structure; 
	Firm consistence; 
	1.9 - 2.1 m	Yellow (10YR7/6-Moist); , 10YR86; Single grain grade of structure; Weak consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	ROBE

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS5	Site ID:	A980	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.8J	 0.084A	 5.8B	 0.7	 0.1	 0.16
	8.1A
	0.03 - 0.1	6.7J	 0.041A	 3.8B	 0.3	 0.05	 0.08
	7.9A
	0.1 - 0.2	4.8J	 0.019A
	6.4A
	0.2 - 0.3	4.1J	 0.014A
	5.6A
	0.3 - 0.4	4.1J	 0.011A
	5.6A
	0.4 - 0.5	4.3J	 0.011A
	6A
	0.5 - 0.6	5.2J	 0.019A	 0.4B	 0.1	 0.02	 0.07
	6.4A
	0.6 - 0.8	4.9J	 0.011A
	6.1A
	0.8 - 0.9	5.4J	 0.014A
	6.3A
	0.9 - 1	5J	 0.011A
	6.2A
	1 - 1.16	4.5J	 0.011A
	5.6A
	1.16 - 1.36	4.5J	 0.014A
	6A
	1.36 - 1.6	4.8J	 0.014A
	6.1A
	1.6 - 1.75	4.9J	 0.011A
	6.3A
	1.75 - 1.9	5J	 0.014A
	6.3A
	1.9 - 2.1	5J	 0.014A
	6.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 0.09C	 0.698A	 4A	 0.044B	 0.1A	 0	 53C	 39	 2	 2
	0.03 - 0.1	 0.02C	 0.581A	 3A	 0.03B	 0.07A	 0	 64C	 33	 0	 2
	0.1 - 0.2	 0.026B	 0.06A	 0	 62C	 36	 2	 1
	0.2 - 0.3
	0.3 - 0.4	 0.008B	 0.07A	 0	 48C	 50	 2	 1
	0.4 - 0.5
	0.5 - 0.6	 0.004B	 0.07A	 0	 39C	 59	 1	 2
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1	 0.001B	 0.09A	 0	 50C	 48	 2	 2
	1 - 1.16
	1.16 - 1.36
	1.36 - 1.6	 0.007B	 0.1A	 0	 37C	 60	 2	 2
	1.6 - 1.75
	1.75 - 1.9	 0.006B	 0.07A	 0	 50C	 47	 2	 2

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS5	Site ID:	A980	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	1.9 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.16
	1.16 - 1.36
	1.36 - 1.6
	1.6 - 1.75
	1.75 - 1.9
	1.9 - 2.1

	Project Name:	1968 ISSS Congress Tour
	Project Code:	IS5	Site ID:	A980	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_C_2.5	pH of soil - pH of 1:2.5 Soil/0.1M CaCl2 suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded