Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A231	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	08/11/55	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	138.945555555556	Runoff:	Very slow
	Easting/Lat.:	-35.4194444444445	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Brown Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized 
	All necessary analytical data are available.	solonetz
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.02 m	Pale brown (10YR6/3-Moist); ; Sandy loam; Massive grade of structure; Firm consistence; 
	Many, fine (1-2mm) roots; Diffuse change to - 
	A2	0.02 - 0.11 m	Light brownish grey (2.5Y6/2-Moist); ; Sandy clay loam; Massive grade of structure; Strong 
	consistence; Sharp change to - 
	B1	0.14 - 0.4 m	Dark grey (10YR4/1-Moist); Dark greyish brown (10YR4/2-Dry); ; Medium clay; Strong grade of 
	structure, 10-20 mm, Angular blocky; Strong grade of structure, 2-5 mm, Angular blocky; Very 
	firm consistence; Diffuse change to - 
	B2	0.4 - 0.53 m	Brown (10YR4/3-Moist); ; Medium clay; 2-5 mm, Angular blocky; Very firm consistence; Diffuse 
	change to - 
	Bk	0.53 - 0.76 m	Brown (10YR4/3-Moist); ; Medium clay; 10-20 mm, Angular blocky; Very firm consistence; 
	Common (10 - 20 %), Calcareous, , Soft segregations; 
	C	0.76 - 1.21 m	Brown (10YR4/3-Moist); ; Medium clay; Few (2 - 10 %), Calcareous, , Soft segregations; 
	C	1.52 - 1.87 m	Red (2.5YR5/8-Moist); ; Sandy clay loam; Very weak consistence; 
	Morphological Notes
	Observation Notes
	LAYER 3 - WORM CASTS & ROOT CHANNELS:                                                                                   
	Site Notes
	CO.HINDMARSH

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A231	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	7.2H	 0.054C
	0.02 - 0.11	7.2H	 0.028C
	0.14 - 0.4	7.7H	 0.047C	 10.2K	 10.4	 1.9	 3.1
	0.4 - 0.53	9.1H	 0.16C
	0.53 - 0.76	9.3H	 0.21C	 1K	 1.9	 0.3	 19.3
	0.76 - 1.21	9.3H	 0.27C
	1.52 - 1.87	9.3H	 0.095C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 0.15B	 24C	 44	 18	 12
	0.02 - 0.11
	0.14 - 0.4	 0.084B	 12C	 18	 10	 58
	0.4 - 0.53	 2.5C
	0.53 - 0.76	 10.1C
	0.76 - 1.21	 3.6C
	1.52 - 1.87	 0.04C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.11
	0.14 - 0.4
	0.4 - 0.53
	0.53 - 0.76
	0.76 - 1.21
	1.52 - 1.87

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A231	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded