Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	19/11/55	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	138.941944444444	Runoff:	No runoff
	Easting/Lat.:	-35.4438888888889	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Class Undetermined Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solonchak
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Mid Strata - Shrub, 1.01-3m, . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	; Clay loam; , Platy; Very weak consistence; Sharp, Irregular change to - 
	0.1 - 0.15 m	; Sandy clay loam; Massive grade of structure; Sharp change to - 
	0.15 - 0.22 m	Light brownish grey (2.5Y6/2-Moist); ; Clayey sand; Single grain grade of structure; Sharp 
	change to - 
	0.24 - 0.34 m	Pale yellow (5Y8/3-Moist); ; Sandy medium clay; Massive grade of structure; Few (2 - 10 %), 
	Calcareous, , Soft segregations; Diffuse change to - 
	0.34 - 0.55 m	; Medium clay; Very plastic; 
	0.55 - 0.66 m	White (5Y8/2-Moist); ; Medium clay; Very plastic; Many (20 - 50 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	LAYER 2 - COXEILLA SHELL LAYER                                                                                          
	Site Notes
	CO.HINDMARSH

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.2H	 4C
	0.1 - 0.15	8.6H	 2C
	0.15 - 0.22	8.7H	 1.4C
	0.24 - 0.34	8.5H	 1.6C
	0.34 - 0.55	8.3H	 2.5C
	0.55 - 0.66	8.4H	 2.4C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.16C	 0.11B	 43C	 21	 2	 26
	0.1 - 0.15	 10C
	0.15 - 0.22	 3.8C
	0.24 - 0.34	 0.07C	 0.009B	 51C	 25	 0	 21
	0.34 - 0.55	 8.1C
	0.55 - 0.66	 27C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.22
	0.24 - 0.34
	0.34 - 0.55
	0.55 - 0.66

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A233	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded