Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	17/11/55	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	139.399722222222	Runoff:	Very slow
	Easting/Lat.:	-35.6547222222222	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Petroclcic Subnatric Black Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized 
	All necessary analytical data are available.	solonetz
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.06 m	Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	AbundantSharp change to - 
	A1	0.06 - 0.17 m	Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	AbundantDiffuse change to - 
	A2	0.21 - 0.3 m	Light grey (2.5Y7/2-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	CommonSharp change to - 
	B1	0.3 - 0.38 m	Yellowish brown (10YR5/6-Moist); ; Sandy medium clay; 200-500 mm, Columnar; Very strong 
	consistence; Diffuse change to - 
	B2	0.38 - 0.5 m	Very dark brown (10YR2/2-Moist); ; Medium clay; Massive grade of structure; Very coarse, (20
	 - 50) mm crack; Very strong consistence; Few
	Bk	0.5 - 0.8 m	; 
	Morphological Notes
	Bk	travertine
	Observation Notes
	DEPTH TO TRAVERTINE VARIES FROM 43-61CM                                                                                 
	Site Notes
	COUNTY RUSSELL

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.8H	 0.017C	 2.4K	 0.6	 0.16	 0.2	 0.5D
	0.06 - 0.17	5.9H	 0.011C
	0.21 - 0.3	6.2H	 0.009C
	0.3 - 0.38	7.6H	 0.046C	 3.3K	 4.5	 2.2	 0.97	 0.47D
	0.38 - 0.5	8.8H	 0.065C
	0.5 - 0.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 0.07B	 44C	 51	 1	 2
	0.06 - 0.17
	0.21 - 0.3
	0.3 - 0.38	 0.033B	 32C	 45	 0	 23
	0.38 - 0.5	 0.02C
	0.5 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.17
	0.21 - 0.3
	0.3 - 0.38
	0.38 - 0.5
	0.5 - 0.8

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A244	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded