Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A249	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-132   1:250000	Rainfall:	0
	Northing/Long.:	139.418611111111	Runoff:	Very slow
	Easting/Lat.:	-35.4577777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Calcarosolic Oxyaquic Hydrosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solonchak
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.02 m	Black (10YR2/1-Moist); ; Clay loam; Very weak consistence; Sharp change to - 
	0.02 - 0.14 m	Black (10YR2/1-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Prismatic; 10-20 
	mm, Angular blocky; Very firm consistence; Common (10 - 20 %), Calcareous, , ; 
	AbundantDiffuse change to - 
	0.14 - 0.3 m	Black (5Y2/1-Moist); ; Medium clay; , Angular blocky; , Angular blocky; Very firm consistence; 
	Common (10 - 20 %), Calcareous, , ; Diffuse change to - 
	0.34 - 0.4 m	Light olive grey (5Y6/2-Moist); ; Sandy clay loam; Massive grade of structure; CommonDiffuse 
	change to - 
	0.4 - 0.45 m	; Many (20 - 50 %), Calcareous, , Soft segregations; Sharp change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	COUNTY RUSSELL

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A249	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.4H	 9C
	0.02 - 0.14	7.6H	 1.1C
	0.14 - 0.3	7.9H
	0.34 - 0.4	8.7H	 0.68C
	0.4 - 0.45
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 0.64B	 17C	 32	 23	 22
	0.02 - 0.14
	0.14 - 0.3	 0.01C	 0.13B	 3C	 6	 13	 67
	0.34 - 0.4	 0.02C	 36C	 49	 12
	0.4 - 0.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.14
	0.14 - 0.3
	0.34 - 0.4
	0.4 - 0.45

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A249	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction