Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A405	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	20/09/56	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-13   1:250000	Rainfall:	0
	Northing/Long.:	139.053611111111	Runoff:	Slow
	Easting/Lat.:	-35.3102777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	0 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Calcic Black Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Very dark grey (7.5YR3/1-Moist); ; Clay loam; , Granular; Weak consistence; Diffuse change to 
	0.1 - 0.2 m	Very dark grey (10YR3/1-Moist); Very dark brown (10YR2/2-Dry); ; Medium clay; , Granular; 
	Weak consistence; Diffuse change to - 
	0.2 - 0.38 m	Very dark grey (10YR3/1-Moist); Very dark brown (10YR2/2-Dry); , 7.5YR32; Medium clay; 
	Strong grade of structure, <2 mm, Angular blocky; Very weak consistence; Diffuse change to - 
	0.38 - 0.68 m	Dark brown (7.5YR3/2-Moist); ; Medium clay; Strong grade of structure, <2 mm, Angular blocky;
	 Very weak consistence; Sharp, Irregular change to - 
	0.68 - 0.83 m	Brown (7.5YR4/2-Moist); ; Medium clay; <2 mm, Angular blocky; Very weak consistence; Few 
	(2 - 10 %), Calcareous, , Concretions; 
	0.83 - 1.06 m	; Medium clay; 
	1.57 - 1.65 m	; Fine sandy medium clay; 
	Morphological Notes
	Observation Notes
	VINE ROOTS TO BOTTOM OF PIT                                                                                             
	Site Notes
	FREELING

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A405	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.8H	 0.063C	 23.7K	 7.2	 1.6	 1.3	 2.6D
	0.1 - 0.2	8.3H	 0.032C
	0.2 - 0.38	8.5H	 0.036C
	0.38 - 0.68	8.5H	 0.068C
	0.68 - 0.83	8.8H	 0.14C
	0.83 - 1.06	8.6H	 0.26C
	1.57 - 1.65	8.2H	 0.34C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.14C	 0.058F	 0.21B
	0.1 - 0.2	<0.01C	 6C	 29	 28	 35
	0.2 - 0.38	<0.01C	 0.065B
	0.38 - 0.68	 0.014C
	0.68 - 0.83	 0.49C
	0.83 - 1.06	 1.24C
	1.57 - 1.65	 0.19C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.38
	0.38 - 0.68
	0.68 - 0.83
	0.83 - 1.06
	1.57 - 1.65

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A405	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded