Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A418	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	J.S. Russel	Locality:
	Date Desc.:	25/09/56	Elevation:	No Data
	Map Ref.:	Sheet No. : SI54-14   1:250000	Rainfall:	0
	Northing/Long.:	139.652777777778	Runoff:	Rapid
	Easting/Lat.:	-35.3402777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	No Data
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Regolithic Bleached Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - , , . *Species includes - Medicago sativa
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Loose consistence; Diffuse 
	change to - 
	A21	0.1 - 0.22 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; 
	A22	0.22 - 0.38 m	Very pale brown (10YR7/4-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	Diffuse change to - 
	B1	0.38 - 0.6 m	Brownish yellow (10YR6/6-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	Sharp change to - 
	B2	0.6 - 0.71 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam (Light); Massive grade of structure; Very 
	weak consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; Sharp change to - 
	0.71 - 0.88 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.88 - 1.06 m	Yellow (10YR7/6-Moist); ; Sand; Single grain grade of structure; Weak consistence; Common 
	(10 - 20 %), Calcareous, , Soft segregations; 
	1.19 - 1.52 m	Very pale brown (10YR7/4-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	Many (20 - 50 %), Calcareous, , Concretions; 
	Morphological Notes
	Observation Notes
	Site Notes
	CO.BUCCLEUCH

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A418	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8H	 0.024C
	0.1 - 0.22	8.3H	 0.021C
	0.22 - 0.38	8.7H	 0.019C
	0.38 - 0.6	9.2H	 0.031C
	0.6 - 0.71	9.1H	 0.044C
	0.71 - 0.88	9.3H	 0.042C
	0.88 - 1.06	9.4H	 0.039C
	1.19 - 1.52	10H	 0.12C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.03C	 0.07B
	0.1 - 0.22	 0.01C
	0.22 - 0.38	 0.02C
	0.38 - 0.6	 0.22C
	0.6 - 0.71	 1.6C	 37C	 46	 1	 14
	0.71 - 0.88	 0.69C
	0.88 - 1.06	 2.1C
	1.19 - 1.52	 8.9C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.22
	0.22 - 0.38
	0.38 - 0.6
	0.6 - 0.71
	0.71 - 0.88
	0.88 - 1.06
	1.19 - 1.52

	Project Name:	Lakes District, S.A.
	Project Code:	LD1	Site ID:	A418	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded