Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A687	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G.G. Beckmann	Locality:
	Date Desc.:	06/08/59	Elevation:	 439 metres
	Map Ref.:	Sheet No. : SI54-9   1:250000	Rainfall:	0
	Northing/Long.:	138.966666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-34.7341666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	Steep hills 90-300m 32-56%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	23 metres
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, 12.01-20m, . *Species includes - Pinus radiata, Eucalyptus species
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Greyish brown (2.5Y5/2-Moist); , 5YR52; Sand; Single grain grade of structure; Very weak 
	consistence; Common
	A2	0.13 - 0.22 m	Grey (5Y5/1-Moist); ; Sand; Single grain grade of structure; Very weak consistence; Few
	B2	0.22 - 0.45 m	Strong brown (7.5YR5/8-Moist); , 10R36; , 5Y63; Medium clay (Heavy); Strong grade of 
	structure, 10-20 mm; Very weak consistence; 
	C	0.45 - 0.53 m	; Firm consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	MT CRAW.FOREST

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A687	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.9H	 0.017C	 2.7K	 1.2	 0.19	 0.16
	0.13 - 0.22	5.9H	 0.008C
	0.22 - 0.45	5.7H	 0.018C	 1.8K	 3.2	 0.19	 0.31
	0.45 - 0.53	5.8H	 0.012C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.8E	 0.015F	 0.086B	 0.04B	 50C	 34	 5	 7
	0.13 - 0.22	 0.028B	 32	 53C	 34	 5	 6
	0.22 - 0.45	 0.57E	 0.039F	 0.039B	 0.51B	 3	 32C	 18	 8	 41
	0.45 - 0.53
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.22
	0.22 - 0.45
	0.45 - 0.53

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A687	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded