Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A733	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	G.G. Beckmann	Locality:
	Date Desc.:	17/05/60	Elevation:	 427 metres
	Map Ref.:	Sheet No. : SI54-9   1:250000	Rainfall:	711
	Northing/Long.:	138.888055555556	Runoff:	Slow
	Easting/Lat.:	-34.7666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	Steep low hills 30-90m 32-56%	Pattern Type:	Hills
	Morph. Type:	Ridge	Relief:	17 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, . *Species includes - Aristida species
	Mid Strata - Tree, 6.01-12m, . *Species includes - Acacia species, Xanthorrhoea species
	Tall Strata - Tree, 12.01-20m, . *Species includes - Pinus radiata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (2.5Y4/2-Moist); ; Loamy sand; Single grain grade of structure; Very weak 
	consistence; Common, fine (1-2mm) roots; 
	A2	0.1 - 0.25 m	Dark greyish brown (2.5Y4/2-Moist); , 10YR65; Clay loam, sandy; Single grain grade of 
	structure; Moist; Very weak consistence; Few, fine (1-2mm) roots; 
	B1	0.25 - 0.36 m	Brownish yellow (10YR6/6-Moist); ; Sandy light clay; Massive grade of structure; Very weak 
	consistence; FewAbrupt change to - 
	B21	0.36 - 0.51 m	; Sandy light clay; Massive grade of structure; Very weak consistence; Gradual change to - 
	B22	0.51 - 0.66 m	Brownish yellow (10YR6/8-Moist); ; , 2.5YR56; Sandy light clay; Massive grade of structure; 
	Very weak consistence; 
	BC	0.71 - 1.22 m	; Sandy clay loam; Massive grade of structure; Very weak consistence; 
	C	1.22 - 1.75 m	; Sandy clay loam; Massive grade of structure; Very weak consistence; 
	1.75 - 1.83 m	; 
	Morphological Notes
	Observation Notes
	SUBSTRATE - WITH BANDS OF QUARTZITE                                                                                     
	Site Notes
	MT CRAW.FOREST

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A733	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	 0.012C	 1.4K	 0.7	 0.17	 0.09
	0.1 - 0.25	5.9A	 0.009C	 0.9K	 0.5	 0.12	 0.07
	0.25 - 0.36	6A	 0.006C
	0.36 - 0.51	5.9A	 0.009C
	0.51 - 0.66	6A	 0.01C	 1.4K	 4.6	 0.11	 0.25
	0.71 - 1.22	5.9A	 0.009C
	1.22 - 1.75	6A	 0.009C
	1.75 - 1.83
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.38E	 0.004F	 0.052B	 4	 18C	 63	 7	 12
	0.1 - 0.25	 0.031B	 4	 17C	 60	 7	 16
	0.25 - 0.36	 2	 16C	 55	 7	 22
	0.36 - 0.51	 11C	 34	 9	 44
	0.51 - 0.66	 0.006F	 0.018B	 7C	 24	 9	 59
	0.71 - 1.22
	1.22 - 1.75	 13C	 49	 13	 23
	1.75 - 1.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.36
	0.36 - 0.51
	0.51 - 0.66
	0.71 - 1.22
	1.22 - 1.75
	1.75 - 1.83

	Project Name:	Mt. Crawford, F.R.
	Project Code:	MC1	Site ID:	A733	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4A1	pH of 1:5 soil/water suspension
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded